SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RNVT60017
	Type ( Engine )
	WagonShape ( RNVT60017.s )
	
	Size  ( 3.09584m 4.20449m 7.47899m )
	CentreOfGravity ( 0.0m 0.0m 0.0m )
	Centre ( 0.00431323m 2.09131m -0.000545979m )
	Mass ( 12.25t )
	InertiaTensor ( Box(3.09584m 4.20449m 7.47899m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e6N/m 1e6N/m )
			Break ( 3.2e6N 3.2e6N )
			r0 ( 20cm 40cm )
		)
	)
	Adheasion ( 0.30 0.76 0.53 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 50kN )
	DerailBufferForce ( 40kN )
	WheelRadius ( 0.4825m )
	NumWheels ( 2 )
	Friction (
		249.5N/m/s -0.1 1.7mph	1.633N/m/s 1.974
		5.1N/rad/s 1 -1rad/s 0 1
	)
	
	BrakeEquipmentType ( "Handbrake, Triple_valve, Auxilary_reservoir" )
 	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce( 16.47kN )
	MaxHandbrakeForce( 5kN )
	NumberOfHandbrakeLeverSteps( 20 )

 TripleValveRatio( 2.5 )
 MaxReleaseRate( 30 )
 MaxApplicationRate( 20 )
 MaxAuxilaryChargingRate( 29 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 21 )
	Sound (	RNVT60017eng.sms )

)

Engine ( RNVT60017
 Effects
 (
  SteamSpecialEffects
  (
   comment
   (
    the format of these little blocks is as follow:

    offset.x offset.y offset.z
    normal.x normal.y normal.z
    width in metres

    defining the offset from the shape pivot point
    where steam / smoke should appear, the direction
    it should go and the width of the nozzle
   )

   SafetyValvesFX
   (
    -0.32 4.00 -0.22
    0 1 0
    0.2
   )

   StackFX
   (
    -0.32 4.00 -0.22
    0 1 0
    0.4
   )

   DrainpipeFX
   (
    -0.32 4.00 -0.22
    -0.4 -1 -0.2
    0.05
   )

   CylindersFX
   (
    -0.32 4.00 -0.22
    0 0 1
    0.05
   )

   CylindersFX
   (
    -0.32 4.00 -0.22
    0 0 1
    0.05
   )
  )
 )


	Wagon ( RNVT60017 )
	IsTenderRequired( -1 )
	
	Type ( Steam )
	MaxPower ( 3kW )
	MaxForce ( 0.01kN )
	MaxVelocity ( 60mph )
	WheelRadius ( 0.5m )
	Sanding ( 1e9mph )
	NumWheels ( 2 )

	BoilerLength ( 0.5m )
	BoilerVolume ( 21.4 )
	BoilerEffectivity ( 1.0 )
	DraftingEffect ( -0.48 )
	BoilerResponsiveness ( 1.0 )
	CoalBurnage ( 1.821lb/hp/h )
	MaxBoilerOutput ( 42lb/h )
	NumCylinders ( 1 )
	CylinderStroke ( 1.97in )
	CylinderDiameter ( 1.97in )
	CylinderVolume ( 0.01 )
	CylinderEffectivity ( 0.53 )

	InjectorSizes ( 11mm 12mm )
	ExhaustLimit ( 25lb/h )
	PrimingFactor ( 1 )
	BlastExponent ( 0.5 )
	MaxBoilerPressure ( 28.45psi )
	MaxFireMass ( 32lb )
	IdealFireMass ( 20lb )
	MaxWaterMass ( 266.5lb )  
	SafetyValvesSteamUsage ( 5lb/h )
	ShovelCoalMass ( 1lb )
	SmokeCombustion ( 1 )
	MaxTenderCoalMass ( 1500lb )
	MaxTenderWaterMass ( 1000lb )

	comment(0 for live steam, 1 for exhaust steam)
	InjectorTypes( 0 1 ) 
	SuperHeater ( 1.0 )
	SteamSmokeUnitsPerPoundOfFuel( 1 )
	SteamMaxSmokeUnitsReleaseRate( 10 )
	MaxSteamHeatingPressure( 80 )
	SafetyValvePressureDifference( 5 )
	SteamGaugeGlassHeight( 1 )
	BasicSteamUsage ( 27lb/h )
	BasicCoalUsage ( 10lb/h )

	comment( min steam pressure, min water proportion, max water proportion  )
	InjectorLimits1 ( 50psi 0.6 1 )
	InjectorLimits2 ( 60psi 0 1 )
	CylinderCocksPowerEfficiency ( 0.9 )
	SteamCylinderCocksOperation( Manual )

     	TrainBrakesControllerMaxReleaseRate( 12 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 21 )

	EngineBrakesControllerHasProportionalBrake( 1 )
      EngineBrakesProportionalBrakeLag( 0.9 )

	CutoffMaxReverse( 55 )
 	CutoffMaxForward( 75 )

	SteamSmallestCutoff( 8 )
	NumberOfDamperSteps( 4 )

	RegulatorValveType( Single_port )
	RegulatorMainValveExponent( 1 )

	SteamBlowerEffectExponent( 0.9 )
	SteamBlowerEfficiencyExponent( 1.1 )
	SteamBlowerMaxSteamUsageRate( 50 )	comment( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect( 0.15 )
	
	SteamSmokeUnitsPerPoundOfFuel( 6.3 )

	CabView ( RNVT60017.cvf )
	HeadOut (  1.7 3.1 -5.5 )

        EngineControllers (
            comment( Engine controls )
        
            Regulator ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.55 0.75 0.01 0 
                NumNotches( 0 )
            )
            Brake_Train ( 0 1 0.01 0.65 
                NumNotches( 3
                    Notch(0     1 TrainBrakesControllerReleaseStart )
                    Notch(0.4   1 TrainBrakesControllerRunningStart )
                    Notch(0.5   1 TrainBrakesControllerApplyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1 
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            WaterScoop ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            Headlights( 0 1 0 )
        )

	comment(fire temp, fire mass, water mass, boiler pressure,
		water level, tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
		
	EngineVariables( 775 20 213.2 28.45 0 0 0 200 1 1 )
    	Sound (	RNVT60017wag.sms )
    	Name ( "RNVT60017" )
 	Description (
 	""

	)
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to increase the Regulator setting.\n"+  
	"4.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n"+
	"2. To hold the brakes at their current setting, lower the brake lever until it's in its middle (Neutral) position, by pressing the ; (SEMICOLON) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press  the ; (SEMICOLON) key to release the train brakes.\n"+
	"2. When the brakes are released, raise the brake lever until it's in its middle (Neutral) position, by pressing the ' (APOSTROPHE) key.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n\n"+
	"To operate the blower\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+ 
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2."
	)
)
