SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN282F0404c
	comment( Class A1 )
	Type ( Engine )
	WagonShape ( RN282-0404c.s )
	Size  ( 3.5m 4.54m 4.75m )
	CentreOfGravity ( 0m 0m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 10t )
	InertiaTensor ( Box(3.5m 4.54m 4.25m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 2e6N/m 9e6N/m )
			Damping ( 1e6N/m 5e6N/m )
			Break ( 1e7N 1e7N )
			r0 ( 180cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Coupling (
		Type ( Bar  )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m 5e6N/m )
			Break ( 1.1e7N 1.1e7N )
			r0 ( 5cm 10cm )
		)
		CouplingHasRigidConnection(1)
	)
	
	Adheasion ( 0.38 0.76 0.83 0 )	
	DerailRailHeight ( 7cm )
	DerailRailForce ( 2.5*10t )
	DerailBufferForce ( 200kN )
	WheelRadius ( 0.47m )
	NumWheels ( 4 )

comment(Fcalc 90kmh, 8 axles, 12M2, 10T, 50T, 1.00)
	Friction (		
		579.7N/m/s -0.10  1.8mph  7.110N/m/s  1.995
		5.1N/rad/s   1	  -1rad/s  0	       1
	)
	
	BrakeEquipmentType( "Triple_Valve, Handbrake, Auxilary_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 9.18kN )
	MaxHandbrakeForce( 5kN )
	NumberOfHandbrakeLeverSteps( 10 )
	TripleValveRatio( 2.5 )		
        MaxReleaseRate( 20 )
        MaxApplicationRate( 20 )
        MaxAuxilaryChargingRate( 30 )
        BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )       
	
	
Lights ( 6
	Light	(
		comment( Luz Roja trasera izq )
		Type		( 0 )
		Conditions	(
			Headlight ( 3 )
			Unit ( 3 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( -1.0 2 -2.65)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
	Light	(
		comment( Luz Roja trasera der )
		Type		( 0 )
		Conditions	(
			Headlight ( 3 )
			Unit ( 3 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( 1.0 2 -2.65)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
	Light	(
		comment( Luz Roja trasera central )
		Type		( 0 )
		Conditions	(
			Headlight ( 3 )
			Unit ( 3 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( 0 3.05 -2.35)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
	Light	(
		comment( Luz Roja trasera AI izq )
		Type		( 0 )
		Conditions	(
			Headlight ( 0 )
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 0 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( -1.0 2 -2.65)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
	Light	(
		comment( Luz Roja trasera AI der )
		Type		( 0 )
		Conditions	(
			Headlight ( 0 )
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 0 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( 1.0 2 -2.65)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
	Light	(
		comment( Luz Roja trasera AI central )
		Type		( 0 )
		Conditions	(
			Headlight ( 0 )
			Unit ( 3 )
			Control ( 1 )
			Service ( 2 )
			TimeOfDay ( 0 )
		)
		FadeIn	( 0.5 )
		FadeOut	( 0.5 )
		Cycle		( 0 )
		States	( 1
			State	(
				Duration ( 0.0 )
				LightColour ( b0ff0000 )
				Position ( 0 3.05 -2.35)
				Azimuth ( -180 -180 -180 )
				Transition ( 0 )
				Radius ( 0.5 )
			)
		)
	)
)

	
Engine ( RN282F0404c
	comment( Class A1 )
	Effects
	(
		SteamSpecialEffects
		(

			StackFX
			(
				0 4.578 12.898
				0 1.4 0
				0.5
			)

			DrainpipeFX
			(
				-1.5 1.258 -3.886
				-0.4 -1 -0.2
				0.05
			)

			CylindersFX
			(
				-1.158 0.321 -1.661
				0 0 -1
				0.25
			)

			CylindersFX
			(
				1.158 0.321 -1.661
				0 0 -1
				0.25
			)
		)
	)

	Wagon ( RN282F0404c )
	IsTenderRequired( -1 )	
	Type ( Steam )
	MaxPower ( 10.0kW )
	MaxForce ( 4.1lbf )
	MaxVelocity ( 12.0mph )
	WheelRadius ( 0.600m )
	Sanding ( 1e9mph )
	NumWheels ( 4 )
	BoilerLength ( 2.05m )
	BoilerVolume ( 5.3 )
	BoilerEffectivity ( 1.00 )
	DraftingEffect ( 1.0953)
	BoilerResponsiveness ( 1.00 )
	CoalBurnage ( 2.98lb/hp/h )
	MaxBoilerOutput ( 9334lb/h )
	ExhaustLimit ( 8668lb/h )
	NumCylinders ( 2 )
	CylinderStroke ( 1.2in )
	CylinderDiameter ( 1.4in )
	CylinderVolume ( 1 )
	CylinderEffectivity ( 1.00 )
	InjectorSizes ( 11mm 12mm )
	PrimingFactor ( 1 )
	BlastExponent ( 0.5 )
	MaxBoilerPressure ( 56.89psi )
	MaxFireMass ( 148lb )
	IdealFireMass ( 100lb )
	MaxWaterMass ( 65.9lb )  
	SafetyValvesSteamUsage ( 4800lb/h )
	ShovelCoalMass ( 1lb )
	SmokeCombustion ( 1 )
	MaxTenderCoalMass ( 4500lb )
	MaxTenderWaterMass ( 11000lb )
	comment(0 for live steam, 1 for exhaust steam)
	InjectorTypes( 0 0 ) 
	SuperHeater ( 1 )
	SteamSmokeUnitsPerPoundOfFuel( 8 )
	SteamMaxSmokeUnitsReleaseRate( .1 )
	MaxSteamHeatingPressure( 80 )
	SafetyValvePressureDifference( 5 )
	SteamFiremanMaxPossibleFiringRate( 1760 )
	SteamGaugeGlassHeight( 4 )

	BasicSteamUsage ( 300lb/h )
	BasicCoalUsage ( 110lb/h )
	comment( min steam pressure, min water proportion, max water proportion  )
	Inyector1WaterValveVariance(.8)
	Inyector2WaterValveVariance(.8)
	InjectorLimits1 ( 50psi 0.2 1 )
	InjectorLimits2 ( 50psi 0.2 1 )
	CylinderCocksPowerEfficiency ( 0.9 )
	SteamCylinderCocksOperation( Manual )
	RegulatorValveType( Single_port )
	RegulatorMainValveExponent( 1 )
	SteamSmallestCutoff( 0.8 )
	NumberOfDamperSteps( 4 )


	SteamBlowerEffectExponent( 0.9 )
	SteamBlowerEfficiencyExponent( 1.1 )
	SteamBlowerMaxSteamUsageRate( 500 )	comment( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect( 0.15 )
	

	AirBrakesAirCompressorPowerRating( 3.93 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 110 )
	AirBrakesMainResVolume( 25 )
	AirBrakesCompressorRestartPressure( 105 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesEngineControllers( "Train, Independent" )
	EngineBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 2.66 )
	EngineBrakesControllerMaxReleaseRate( 20 )
	EngineBrakesControllerEmergencyApplicationRate( 7.7 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 60 )
	EngineBrakesControllerFullServicePressureDrop( 26 )
	EngineBrakesControllerDirectControlExponent( 1 )

	BrakesTrainBrakeType( "Air_single_pipe" )
	TrainBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMaxApplicationRate( 2.66 )
	TrainBrakesControllerMaxReleaseRate( 2.66 )
	TrainBrakesControllerEmergencyApplicationRate( 7.7 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerFullServicePressureDrop( 26 )
	


	comment(fire temp, fire mass, water mass, boiler pressure,
		water level, tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables( 950 220 52.7 56.89 0 0 0 200 1 )		

Sound ( " 282cab.sms " )

    	Name ( "RENFE 282F0404 Trasera" )
 	Description (
 	"Locomotora Garratt para mercancias del Ferrocarril Central de Aragón version RENFE fuelizada. Fue construida por Babcock & Wilcox en 1931"+ 
 	"Esta es la parte TRASERA de la locomotora. Para montarla entera hay que unir las partes A, B y C" 
)

)