SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN040-2302
	Type ( Engine )
	WagonShape ( RN040-2302.s )

	Size  ( 3.16m 4.42m 9.7m )
	CentreOfGravity ( 0m 1.86m 0m )
	Centre ( 0m 0m 0m )
	Mass ( 50.21t )
	InertiaTensor ( Box(3.16m 4.42m 9.2m) )
	Comment ( Use on cars with close coupled no slack couplers ie: passenger cars, roadrailers )
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 6e6N/m 6e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0.1cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.2m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 6e6N/m 6e6N/m )
			Damping ( 1.77e6N/m/s 1.77e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 95cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 9.8e5N/m 9.8e5N/m )
			Damping ( 1.7e6N/m/s 1.7e6N/m/s )
			r0 ( 20cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	
	Adheasion ( 0.30 0.76 1.05 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 218kN )
	DerailBufferForce ( 349kN )
	WheelRadius ( 0.61m )
	NumWheels ( 8 )
	Friction (
		853N/m/s		0		1mph		16.07N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce( 68.93kN )
	MaxHandbrakeForce( 50kN )
	NumberOfHandbrakeLeverSteps( 100 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 15 )
	MaxAuxilaryChargingRate( 15 )
      BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

	

	Lights (	6
		Light	(
			Type		( 1 )
			Conditions	(
					Headlight ( 3 )
					Unit ( 2 )
			)
			Cycle		( 0 )
			FadeIn	( 2.8 )
			FadeOut	( 2.8 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffffffff )
					Position ( 0 3.28 3.77 )
					Transition ( 0 )
					Radius ( 200.0 )
					Angle ( 75.0 )
				)
			)
		)
                                                Light	(
                                                comment( Luz frontal principal )
			Type	( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn	( 2.8 )
			FadeOut	( 2.8 )
			Cycle	( 0 )
			States	(	4
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( 0 3.28 3.77 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.7 )
				)
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( 0 3.28 3.77 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.6 )
				)
				State	(
					Duration ( 0.4 )
					LightColour ( aaffff99 )
					Position ( 0 3.28 3.77 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.9 )
				)
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( 0 3.28 3.77 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.07 )
					Radius ( 0.8 )
				)
			)
		)
		Light	(
			Type	( 0 #Front Left lamp A )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn	( 2.8 )
			FadeOut	( 2.8 )
			Cycle	( 0 )
			States	(	4
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.7 )
				)
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.6 )
				)
				State	(
					Duration ( 0.4 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.9 )
				)
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.07 )
					Radius ( 0.8 )
				)
			)
		)
		Light	(
			Type	( 0 #Front Left lamp B )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn	( 2.8 )
			FadeOut	( 2.8 )
			Cycle	( 0 )
			States	(	4
				State	(
					Duration ( 0.3 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.7 )
				)
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.6 )
				)
				State	(
					Duration ( 0.4 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.9 )
				)
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( -0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.07 )
					Radius ( 0.8 )
				)
			)
		)

		Light	(
			Type	( 0 #Front Right lamp A )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn	( 2.5 )
			FadeOut	( 2.5 )
			Cycle	( 0 )
			States	(	4
				State	(
					Duration ( 0.3 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.7 )
				)
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.6 )
				)
				State	(
					Duration ( 0.4 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.03 )
					Radius ( 0.9 )
				)
				State	(
					Duration ( 0.2 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.290 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.8 )
				)
			)
		)
		Light	(
			Type	( 0 #Front Right lamp B )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
			)
			FadeIn	( 2.8 )
			FadeOut	( 2.8 )
			Cycle	( 0 )
			States	(	4
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.7 )
				)
				State	(
					Duration ( 0.1 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.05 )
					Radius ( 0.5 )
				)
				State	(
					Duration ( 0.4 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.04 )
					Radius ( 0.9 )
				)
				State	(
					Duration ( 0.3 )
					LightColour ( aaffff99 )
					Position ( 0.999 1.520 4.241 )
					Azimuth ( 0.0 -5.0 5.0 )
					Transition ( 0.03 )
					Radius ( 0.8 )
				)
			)
		)
	)	
       
	Sound ("RN040-2301eng.sms")

)

Engine ( RN040-2302  
Effects
	(
		SteamSpecialEffects
		(
			comment
			(
				the format of these little blocks is as follow:

				offset.x offset.y offset.z
				normal.x normal.y normal.z
				width in metres

				defining the offset from the shape pivot point
				where steam / smoke should appear, the direction
				it should go and the width of the nozzle
			)

			WhistleFX
			(
				0 3.75 -3.434
				0 1 0
				0.2
			)

			SafetyValvesFX
			(
				0 4.15 0.550
				0 1 0
				0.3

			)

			StackFX
			(
				0 4.46 3.03
				0 1 0
				0.5
			)

			DrainpipeFX
			(
				-1.5 0.758 -3.806
				-0.4 -1 -0.2
				0.15
			)

			CylindersFX
			(
				-1.013 0.349 3.307
				-1 0 0
				0.25
			)

			CylindersFX
			(
				1.013 0.349 3.307
				1 0 0
				0.25
			)
		)
	)
	Wagon ( RN040-2302 )
	Type ( Steam )
	IsTenderRequired( 1 )
	MaxPower ( 577.2kW )
	MaxForce ( 115.51kN )
	MaxVelocity ( 35mph )
	WheelRadius ( 0.647m )
	Sanding ( 1e9mph )
	NumWheels ( 4 )
	ORTSSteamLocomotiveType( Simple )

Comment ( Boiler )

	BoilerLength ( 3.98m )
	BoilerVolume ( 315.7 )
	BoilerEffectivity ( 1.05 )
	BoilerResponsiveness ( 1 )
	CoalBurnage ( 5.38lb/hp/h )
	MaxBoilerOutput ( 23378lb/h )
	ExhaustLimit ( 20707lb/h )
	MaxBoilerPressure ( 142.23psi )
	SuperHeater ( 1 )
	SafetyValvesSteamUsage ( 12000lb/h )
	SafetyValvePressureDifference( 2 )
	ORTSSteamBoilerType( Saturated )
	ORTSEvaporationArea( 1334.7ft^2 )
	ORTSGrateArea( 26.05ft^2 )
	ORTSBoilerEvaporationRate ( 16.27 )

Comment ( Priming )

	PrimingFactor ( 1 )
	SteamMinPrimingLevel ( 1 )
	SteamPrimingPowerLossProportion ( 0.9 )
	SteamPrimingWaterUsageIncreaseProportion ( 5 )
	SteamPrimingReductionWithCylinderCocksOpen ( 0.5 )

Comment ( Cylinders )

	NumCylinders ( 2 )
	CylinderStroke ( 25.98in )
	CylinderDiameter ( 20in )
	CylinderVolume ( 18.9 )
	CylinderEffectivity ( 1.4 )
	CylinderCocksPowerEfficiency ( 0.8 )
	SteamCylinderCocksOperation( Manual )
	ORTSCylinderEfficiencyRate ( 1 )
	ORTSCylinderPortOpening ( 0.075 ) 
	ORTSBurnRate( 0lb/h, 10lbs/h
				2670.0lb/h, 260.5lbs/h
				6529.0lb/h, 695lbs/h
				9344.0lb/h, 1042lbs/h
				11862.0lb/h, 1389lbs/h
				14092.0lb/h, 1737lbs/h
				16018.0lb/h, 2084lbs/h
				17647.0lb/h, 2431lbs/h
				18986.0lb/h, 2779lbs/h
				20022.0lb/h, 3126lbs/h
				20762.0lb/h, 3473lbs/h
				21210.0lb/h, 3821lbs/h
				21357.0lb/h, 4168lbs/h ) 

Comment ( Fuel and Usage )

	MaxFireMass ( 833.6lb )
	IdealFireMass ( 521lb )
	MaxWaterMass ( 3934.3lb )
	BasicSteamUsage ( 650lb/h )
	BasicCoalUsage ( 260.5lb/h )
	ShovelCoalMass ( 2lb )
	SteamFiremanMaxPossibleFiringRate( 4168 )
	ORTSSteamFiremanMaxPossibleFiringRate( 4168 )
	MaxTenderCoalMass ( 6614lb )
	MaxTenderWaterMass ( 19842lb )
	SteamGaugeGlassHeight( 8 )
	ORTSFuelCalorific( 13000btu/lb )

Comment ( Smoke and Steam )

	SteamMaxSmokeUnitsReleaseRate( 3 )
	SteamSmokeUnitsPerPoundOfFuel( 6.3 )
	MaxSteamHeatingPressure( 80 )
	SmokeCombustion( 1 )

Comment ( Injectors )

	InjectorTypes( 0 1 )
	InjectorSizes( 14mm 14mm )
	Injector1FeedrateMultiplierLive( 0.4 )
	Injector2FeedrateMultiplierExhaust( 0.2 )
	Injector1WaterValveVariance( 0.35 )
	Injector2WaterValveVariance( 0.35 )
	InjectorLimits1 ( 60psi 0.5 1 )  
	InjectorLimits2 ( 60psi 0.5 1 )

Comment ( Regulator and Reverser )

	CutoffMaxReverse( -0.60 )
	CutoffMaxForward( 0.75 )
	SteamSmallestCutoff( 0.8 )
	RegulatorValveType ( single_port )
	RegulatorPilotValveExponent( 1.7 )
	RegulatorPilotValveFullOpenning( 0.49 )
	RegulatorMainValveInitialOpenning( 0.495 )

Comment ( Draft and Blast )

	SteamBlowerEffectExponent( 0.8 )
	SteamBlowerEfficiencyExponent( 1.1 )
	SteamBlowerMaxSteamUsageRate( 700 )
	SteamBlowerMaxProportionOfBlastEffect( 0.3 )
	BlastExponent ( 0.5 )
	DraftingEffect ( 1.12 )
	NumberOfDamperSteps( 4 )

Comment ( Brake Settings )
	
	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
      BrakesEngineControllers( "Hand, Train, Independent" )

   	AirBrakesAirCompressorPowerRating( 3 )
    	AirBrakesMainMinResAirPressure( 0 )
    	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 8 )
    	AirBrakesCompressorRestartPressure( 90 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )

	TrainBrakesControllerMaxApplicationRate( 4 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	TrainBrakesControllerMaxQuickReleaseRate( 6 )
	TrainBrakesControllerEmergencyApplicationRate( 10 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 70 )

    	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesControllerMaxApplicationRate( 6 )
	EngineBrakesControllerMaxReleaseRate( 6 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 70 )


	CabView ( RN040-2301.cvf )
	HeadOut (  1.7 3.1 -5.5 )

        EngineControllers (
            Regulator ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.60 0.75 0.015 0 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.0125 0
                NumNotches( 3
                    Notch(0    1 EngineBrakesControllerReleaseStart )
                    Notch(0.45 1 EngineBrakesControllerHoldStart )
                    Notch(0.5  1 EngineBrakesControllerApplyStart )
                )
            )            
            Brake_Train ( 0 1 0.02 0.4 
                NumNotches( 5
			  Notch(0    0 TrainBrakesControllerFullQuickReleaseStart )
                    Notch(0.2  0 TrainBrakesControllerReleaseStart )
                    Notch(0.4  0 TrainBrakesControllerNeutralhandleOffStart )
                    Notch(0.6  1 TrainBrakesControllerApplyStart )
                    Notch(1.0  0 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables( 800 521.0 3147.4 142.23 0 0 0 200 1 )

    	Sound ("RN040-2301wag.sms")
    	Name ( "RN040-2302" )
 	Description (
 	""

	)
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to increase the Regulator setting.\n"+  
	"4.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n"+
	"2. To hold the brakes at their current setting, lower the brake lever until it's in its middle (Neutral) position, by pressing the ; (SEMICOLON) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press  the ; (SEMICOLON) key to release the train brakes.\n"+
	"2. When the brakes are released, raise the brake lever until it's in its middle (Neutral) position, by pressing the ' (APOSTROPHE) key.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n\n"+
	"To operate the blower\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+ 
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2."
	)
)
