SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN040-2301T
	Type ( tender )
	WagonShape ( RN040-2301T.s )
 	
	Size ( 2.92m 3.17m 5.9m )
	Mass ( 22.396t )
	WheelRadius ( 33in/2 )
	InertiaTensor ( Box (2.92m 3.17m 5.4m) )
	comment ( MSTS Route_Riter Special short car coupler values contributed by Joe Morris and Bill Prieger )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e4N/m 4.5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 30cm 20cm )
		)
		Comment ( CouplingHasRigidConnection ( 1 ) )
		Velocity ( 0.2m/s )
	)
	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 1e4N/m 4.5e6N/m )
			Damping ( 2e6N/m/s 2e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 1cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( -0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 2 )
		Angle ( 10.5deg )
	)

 BrakeEquipmentType ( "Handbrake, Triple_valve, Auxilary_reservoir" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce( 8.4kn )
 MaxHandbrakeForce( 10kN )
 MaxReleaseRate( 20 )
 MaxApplicationRate( 20 )
 MaxAuxilaryChargingRate( 25 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )
 IntakePoint ( -1.9 2.0 FuelWater )
 IntakePoint ( 0 2.0 FuelCoal )

 Adheasion ( 0.2 0.4 2 0 )
 DerailRailHeight ( 10cm )
 DerailRailForce (2.5*22.396t )
 DerailBufferForce ( 800kN )
 WheelRadius ( 0.51m )
 NumWheels ( 2 )
 
	Friction (
		450.8N/m/s    -0.10    1.7mph    1.348N/m/s    1.920
		5.1N/rad/s	1	-1rad/s		0	 1
		)
comment( FCalc 70kmh, 3 axles, 7.0 M2, 28.4tons)

 Lights ( 1

  Light (
   comment( Rear red light center )
   Type  ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 3 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.0 1.66 -3.02 )
     Azimuth ( -180 -180 -180 )
     Transition ( 0 )
     Radius ( 1.0 )
     )
    )
   )
  )
 
  
 Sound ( "genfreightwag1.sms" )
)

