SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN140-2107
	Type ( Engine )
	WagonShape ( RN140-2107.s )
    FreightAnim ( RN140FA.s 1 1 ) 
	Size ( 3.56m 4.52m 11.85m ) 
	CentreOfGravity ( 0.0m 0.0m 0.0m ) 
	Centre ( -0.000239m 2.103m -0.0227m ) 
	Mass ( 77.49t ) 
	InertiaTensor (	Box ( 3.56m 4.52m 11.35m ) 	)

	Coupling ( 	
	    Type ( Bar )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0.1cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Coupling ( 	
	    Type ( Automatic )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( -145cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	   
 
	Adheasion ( 0.30 0.76 0.88 0 ) 
	DerailRailHeight ( 4cm ) 
	DerailRailForce ( 240kN ) 
	DerailBufferForce ( 400kN ) 
	WheelRadius ( 0.78m ) 
	NumWheels ( 4 ) 
	_FCalc ( 35mph roller bearings Cd:1 )
	Friction ( 
		1009.9N/m/s 	-0.10 	1.4mph 	10.506N/m/s 	1.860 
		5.1N/rad/s 	1 	-1rad/s 	0 	1 
	) 
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType ( "Air_single_pipe" ) 
	MaxBrakeForce ( 88.54kN ) 
	MaxHandbrakeForce ( 60kN ) 
	NumberOfHandbrakeLeverSteps ( 100 ) 
	MaxReleaseRate ( 20 ) 
	MaxApplicationRate ( 20 ) 
	MaxAuxilaryChargingRate ( 30 ) 
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 70 ) 

	Sound ( "RN140-2107eng.sms" )
 
	Lights ( 7 
		Light ( 
			comment ( Sphere of light )
			Type ( 1 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			Cycle ( 0 ) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 60FFFF00 ) 
					Position ( 0 3.22 4.78 ) 
					Transition ( 0 ) 
					Radius ( 80.0 ) 
					Angle ( 15.0 ) 
				) 
			) 
		) 
		Light ( 
			comment ( Head light bright )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( FFFFFFCC ) 
					Position ( 0 3.22 4.78 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
		Light ( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 80FFFFCC ) 
					Position ( 0 3.22 4.957 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
		Light ( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 80FFFFCC ) 
					Position ( 0.98 1.420 5.40 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
		Light ( 
			comment ( Head light bright )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 80FFFFCC ) 
					Position ( 0.98 1.420 5.40 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
Light ( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 80FFFFCC ) 
					Position ( -0.98 1.420 5.40 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
		Light ( 
			comment ( Head light bright )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( 80FFFFCC ) 
					Position ( -0.98 1.420 5.40 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
				) 
			) 
		) 
	) 
	Inside ( 
		PassengerCabinFile ( RN140-2107.s ) 
		PassengerCabinHeadPos ( 1.216 3.29 -7.2 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 -20 0 ) 
		Sound ( "RN140-2107eng.sms" ) 
	) 
	Inside ( 
		PassengerCabinFile ( RN140-2107.s ) 
		PassengerCabinHeadPos ( -1.216 3.29 -7.2 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 20 0 ) 
		Sound ( "RN140-2107eng.sms" ) 
	)
	Inside ( 
		PassengerCabinFile ( RN140-2107.s ) 
		PassengerCabinHeadPos ( 0 3.29 -5.5 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 180 0 ) 
		Sound ( "RN140-2107eng.sms" ) 
	)
		
) 

Engine ( RN140-2107 
	Effects ( 
		SteamSpecialEffects ( 
			WhistleFX ( 0 4.35 -3.81 0 1 0 0.2 ) 
			SafetyValvesFX ( 0 4.35 -3 0 1 0 0.2 ) 
			StackFX ( 0 4.29 3.919 0 1 0 0.2 ) 
			DrainpipeFX ( -1.5 1.258 -3.886 -0.4 -1 -0.2 0.05 ) 
			CylindersFX ( -1.53 0.748 2.651 -0.5 0 0 0.15 ) 
			CylindersFX ( 1.53 0.748 2.651 0.5 0 0 0.15 ) 
		) 
	) 
	Wagon ( RN140-2107 )

	Comment ( "Características básicas" )	
 
	IsTenderRequired ( 1 ) 
	Type ( Steam ) 
	MaxPower ( 1024.7kW ) 
	MaxForce ( 164.17kN ) 
	MaxVelocity ( 50mph ) 
	WheelRadius ( 0.78m ) 
	Sanding ( 1e9mph ) 
	NumWheels ( 4 )
	ORTSSteamLocomotiveType ( Simple ) 

	Comment ( "Descripción de la caldera" )

	BoilerLength ( 5.2m ) 
	BoilerVolume ( 420.6 ) 
	BoilerEffectivity ( 1.0 ) 
	DraftingEffect ( 1.1 ) 
	BoilerResponsiveness ( 1.0 ) 
	CoalBurnage ( 3.66lb/hp/h ) 
	MaxBoilerOutput ( 28234lb/h )
	MaxBoilerPressure ( 170.68psi ) 
	ORTSSteamBoilerType ( Superheated )
	ORTSMaxSuperheatTemperature ( 482 )
	ORTSGrateArea ( 3.05m^2 )
	ORTSEvaporationArea ( 184.5m^2 )
	ORTSSuperheatArea ( 46.65m^2 )
	ORTSBoilerEvaporationRate ( 11.65 )
	ORTSBoilerEfficiency ( 5.0 0.90  160.0 0.60 )
	ORTSBurnRate ( 0.0 10.0  3355.76 328.3  7842.5 837.0  11233.6  1256.0  14259.2 1674.0  16936.8 2093.0  19249.9 2511.0  21214.2 2930.0  22821.5 3349.0  24065.6 3767.0  24959.5 4186.0  25491.7 5023.0 ) 

	Comment ( "Cilindros" )

	NumCylinders ( 2 ) 
	CylinderStroke ( 25.59in ) 
	CylinderDiameter ( 24.02in ) 
	CylinderVolume ( 26.83 ) 
	CylinderEffectivity ( 1.28 ) 
	InjectorSizes ( 11mm 12mm ) 
	ExhaustLimit ( 25122lb/h ) 
	PrimingFactor ( 1 ) 
	BlastExponent ( 0.5 ) 
	ORTSCylinderEfficiencyRate ( 1 )
	
	Comment ( "Combustión" )
	
	MaxFireMass ( 1050.6lb ) 
	IdealFireMass ( 656.6lb ) 
	MaxWaterMass ( 5241.2lb ) 
	SafetyValvesSteamUsage ( 14400lb/h ) 
	ShovelCoalMass ( 1lb ) 
	SmokeCombustion ( 1 )
	SteamFiremanMaxPossibleFiringRate ( 5023 ) 
	ORTSFuelCalorific ( 13000btu/lb )
	ORTSSteamFiremanMaxPossibleFiringRate ( 4500 ) 
 
	MaxTenderCoalMass ( 13228lb ) 
	MaxTenderWaterMass ( 30865lb ) 
	comment (0 for live steam, 1 for exhaust steam)
	InjectorTypes ( 0 1 ) 
	SuperHeater ( 1.32 ) 
	SteamSmokeUnitsPerPoundOfFuel ( 1 ) 
	SteamMaxSmokeUnitsReleaseRate ( 10 ) 
	MaxSteamHeatingPressure ( 80 ) 
	SafetyValvePressureDifference ( 5 ) 
	SteamGaugeGlassHeight ( 10 )
 
	BasicSteamUsage ( 550lb/h ) 
	BasicCoalUsage ( 328.3lb/h )
	
	comment ( min steam pressure, min water proportion, max water proportion  )
	InjectorLimits1 ( 50psi 0.6 1 ) 
	InjectorLimits2 ( 60psi 0 1 ) 
	CylinderCocksPowerEfficiency ( 0.8 ) 
	SteamCylinderCocksOperation ( Manual )
 
	RegulatorValveType ( Single_port ) 
	RegulatorMainValveExponent( 1 ) 

	SteamBlowerEffectExponent ( 0.9 ) 
	SteamBlowerEfficiencyExponent ( 1.1 ) 
	SteamBlowerMaxSteamUsageRate ( 500 ) 
	comment ( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect ( 0.15 )  
	SteamSmokeUnitsPerPoundOfFuel ( 6.3 )

	Comment ( "Frenos. Configurados de aire comprimido para ser compatibles con el material remolcado." )

	AirBrakesAirCompressorPowerRating( 3.93 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxAirPressure( 110 )
	AirBrakesMainResVolume( 25 )
	AirBrakesCompressorRestartPressure( 105 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerMinPressureReduction( 6 )
	TrainBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 2.667 )
	TrainBrakesControllerMaxApplicationRate( 2.667 )
	EngineBrakesControllerMaxReleaseRate( 20 )
	TrainBrakesControllerMaxReleaseRate( 2.667 )
	EngineBrakesControllerEmergencyApplicationRate( 7.7 )
	TrainBrakesControllerEmergencyApplicationRate( 7.7 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 90 )
	TrainBrakesControllerMaxSystemPressure( 90 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 60 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )
	EngineBrakesControllerFullServicePressureDrop( 26 )
	TrainBrakesControllerFullServicePressureDrop( 26 )
	
	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
	BrakesEngineControllers( "Train, Independent" )

	EngineBrakesControllerDirectControlExponent( 1 )
 
	CabView ( "RN140-2107.cvf" ) 
	HeadOut ( 1.7 3.4 -5.5 )
 
	EngineControllers ( 
		comment ( Engine controls )
		Regulator ( 0 1 0.025 0 
			NumNotches ( 0 
			) 
		) 
		Cutoff ( -0.75 0.75 0.01 0 
			NumNotches ( 0 
			) 
		) 
		Brake_Train ( 0 1 0.02 0.65 
			NumNotches ( 3 
				Notch ( 0 1 TrainBrakesControllerReleaseStart ) 
				Notch ( 0.3 1 TrainBrakesControllerRunningStart ) 
				Notch ( 0.5 1 TrainBrakesControllerApplyStart ) 
			) 
		)

		Brake_Engine ( 0 1 0.04 0
                NumNotches( 3
                    Notch(0   1 EngineBrakesControllerReleaseStart )
                    Notch(0.4 1 EngineBrakesControllerApplyStart )
		    Notch(0.8 1 EngineBrakesControllerEmergencyStart )
                )
            )            
 
		Brake_Hand ( 0 1 0.0125 0 
			NumNotches ( 0 
			) 
		) 
		FireDoor ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Sanding ( 0 1 0 ) 
		Blower ( 0 1 0.025 0.2 
			NumNotches ( 0 
			) 
		) 
		HeatingTap ( 0 1 0.025 0 
			NumNotches ( 0 
			) 
		) 
		Shovel ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		DampersFront ( 0 1 0.1 1 
			NumNotches ( 0 
			) 
		) 
		DampersBack ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Injector1Steam ( 0 1 0 ) 
		Injector2Steam ( 0 1 0 ) 
		Injector1Water ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Injector2Water ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		CylinderCocks ( 0 1 1 ) 
		Whistle ( 0 1 0 ) 
		Waterscoop ( 0 1 0 ) 
		SmallEjectorOrCompressor ( 0 1 1 ) 
		HeadLights ( 0 1 0 ) 
	) 
	comment (fire temp, fire mass, water mass, boiler pressure,
		water level, tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables ( 900 656.6 4192.9 170.68 0 30865 13228 200 1 1 ) 
	Sound ( "RN140-2107cab.sms" ) 
	Name ( "RN140-2107" ) 
	Description ( "Locomotora " ) 
	EngineOperatingProcedures ( "To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to increase the Regulator setting.\n"+  
	"4.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n"+
	"2. To hold the brakes at their current setting, lower the brake lever until it's in its middle (Neutral) position, by pressing the ; (SEMICOLON) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press  the ; (SEMICOLON) key to release the train brakes.\n"+
	"2. When the brakes are released, raise the brake lever until it's in its middle (Neutral) position, by pressing the ' (APOSTROPHE) key.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n\n"+
	"To operate the blower\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+ 
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2." ) 
) 