SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN140-2505
	Type ( Engine )
	WagonShape ( RN140-2505.s )
    FreightAnim ( RN140FA.s 1 1 ) 
	
	Size ( 3.19m 4.58m 12.1m ) 
	CentreOfGravity ( 0.0m 0.0m 0.0m ) 
	Centre ( -0.000239m 2.103m -0.0227m ) 
	Mass ( 82.1t ) 
	InertiaTensor (	Box ( 3.19m 4.58m 11.6m ) 	)

	Coupling ( 	
	    Type ( Bar )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 20cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Coupling ( 	
	    Type ( Automatic )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	   
 
	Adheasion ( 0.30 0.76 0.88 0 ) 
	DerailRailHeight ( 4cm ) 
	DerailRailForce ( 240kN ) 
	DerailBufferForce ( 400kN ) 
	WheelRadius ( 0.78m ) 
	NumWheels ( 4 ) 
	_FCalc ( 35mph roller bearings Cd:1 )
	Friction ( 
		1009.9N/m/s 	-0.10 	1.4mph 	10.506N/m/s 	1.860 
		5.1N/rad/s 	1 	-1rad/s 	0 	1 
	) 
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType ( "Air_single_pipe" ) 
	MaxBrakeForce ( 94.73kN )
 
	MaxHandbrakeForce ( 32.203kN ) 
	NumberOfHandbrakeLeverSteps ( 100 )
	TripleValveRatio ( 2.5 )
	EmergencyResVolumeMultiplier ( 1 ) 
	MaxReleaseRate ( 15 ) 
	MaxApplicationRate ( 15 ) 
	MaxAuxilaryChargingRate ( 15 )
	EmergencyResChargingRate ( 15 )
	EmergencyResCapacity ( 1.241ft^3 ) 
	BrakeCylinderPressureForMaxBrakeBrakeForce ( 70 ) 

	Sound ( "RN140SMeng.sms" )
 
	Lights ( 6 

		Light	( 
			comment ( Sphere of light )
			Type ( 1 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			Cycle ( 0 ) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( 0 3.22 5.78 ) 
					Transition ( 0 ) 
					Radius ( 200.0 ) 
					Angle ( 15.0 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Head light bright )
			Type ( 0 ) 
			Conditions ( 
				Headlight ( 3 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( 0 3.66 5.13 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( -0.01 3.27 4.89 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.35 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( 1.01 1.55 5.60 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.35 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Head light dim )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 2 ) 
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( -1.01 1.55 5.60 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.35 ) 
					) 
				) 
			) 

comment(        luces IA       )

		Light	( 
			comment ( Head light bright )
			Type ( 0 ) 
			Conditions ( 
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 )
				TimeOfDay ( 0 )
			) 
			FadeIn ( 0.9 ) 
			FadeOut ( 0.9 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffbc49 ) 
					Position ( 0 3.66 5.13 ) 
					Azimuth ( 0.0 0.0 5.0 ) 
					Transition ( 0 ) 
					Radius ( 0.85 ) 
					) 
				) 
			) 
		)
		
comment ( === Vistas interiores desde cabina con tecla 5 y 5 + Mayúsculas === )
		
	Inside (  
		PassengerCabinHeadPos ( 1.216 3.29 -7.2 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 -20 0 ) 
		Sound ( "RN140SMeng.sms" ) 
	) 
	Inside ( 
		PassengerCabinHeadPos ( -1.216 3.29 -7.2 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 20 0 ) 
		Sound ( "RN140SMeng.sms" ) 
	)
	Inside (  
		PassengerCabinHeadPos ( 0 3.29 -5.5 ) 
		RotationLimit ( 180 180 180 ) 
		StartDirection ( 0 180 0 ) 
		Sound ( "RN140SMeng.sms" ) 
	)
	
	
	
	       comment ( === Efectos especiales vapor sección Wagon === )
							   
		Effects (
            SpecialEffects ( 						    			
				comment (escape vapor silbato)
		        WagonSmokeFX (   
			      0.65 4.2 -3.95
                  0 1 0
                  0.03
				)
				comment (escape vapor grifo desague)
				WagonSmokeFX (   
			      1.55 0.85 -5.2
                  0 1 0
                  0.07
				)
				comment (escape vapor grifo desague)
				WagonSmokeFX (   
			      -1.55 0.85 -5.2
                  0 1 0
                  0.07
				)
				comment (válvula de seguridad 1)
				WagonSmokeFX (
				0 4.05 -2.8
				0 1 0
				0.03
		      	)
				comment (válvula de seguridad 2)
				WagonSmokeFX (
				0 4.05 -3.1
				0 1 0
				0.03
		      	)	
                comment (Dinamo)
				WagonSmokeFX (
				-0.9 3.7 -2.9
				0 1 0
				0.03
		      	)					
				comment (cilindros derecha inf)
				WagonSmokeFX (   
			      1.35 0.2 2.75
                  0.5 2 0
                  0.08
				)
				comment (cilindros izquierda inf)
				WagonSmokeFX (   
			      -1.35 0.2 2.75
                  -0.5 2 0
                  0.08
				)
				comment (cilindros derecha sup)
				WagonSmokeFX (   
			      1.3 0.6 2.2
                  0 1 0
                  0.08
				)
				comment (cilindros izquierda sup)
				WagonSmokeFX (   
			      -1.3 0.6 2.2
                  0 1 0
                  0.08
				)
		    )	  
        ) 
		
)

Engine ( RN140-2505 
	Effects ( 
		SteamSpecialEffects ( 
			WhistleFX ( 0.65 4.2 -3.95 0 1 0 0.1 ) 
			SafetyValvesFX ( 0 4.05 -2.8 0 1 0 0.2 ) 
			SafetyValvesFX ( 0 4.05 -3.1 0 1 0 0.15 )
			StackFX ( 0 4.29 3.919 0 1 0 0.2 ) 
			DrainpipeFX ( -1.55 0.85 -5.2 -0.4 -1 -0.2 0.07 ) 
			CylindersFX ( -1.2 0.3 2.75 -0.2 0 0 0.3 ) 
			CylindersFX ( 1.2 0.3 2.75 0.2 0 0 0.3 ) 
		) 
	) 
	Wagon ( RN140-2505 )

	Comment ( "Características básicas" )	
 
	IsTenderRequired ( 1 ) 
	Type ( Steam ) 
	MaxPower ( 1118.7kW ) 
	MaxForce ( 177.74kN ) 
	MaxVelocity ( 55mph ) 
	WheelRadius ( 0.78m ) 
	Sanding ( 1e9mph ) 
	NumWheels ( 4 )
	ORTSSteamLocomotiveType ( Simple ) 

	Comment ( "Descripción de la caldera" )

	BoilerLength ( 5.5m ) 
	BoilerVolume ( 576.3 ) 
	BoilerEffectivity ( 1.0 ) 
	DraftingEffect ( 1.08 ) 
	BoilerResponsiveness ( 1.0 ) 
	CoalBurnage ( 4.02lb/hp/h ) 
	MaxBoilerOutput ( 30893.0lb/h )
	ExhaustLimit ( 30143.0lb/h )
	BlastExponent ( 0.5 ) 
	MaxBoilerPressure ( 199.13psi ) 
	ORTSSteamBoilerType ( Superheated )
	ORTSMaxSuperheatTemperature ( 482 )
	ORTSGrateArea ( 3.5m^2 )
	ORTSEvaporationArea ( 196.0m^2 )
	ORTSSuperheatArea ( 52.0m^2 )
	ORTSBoilerEvaporationRate ( 10.95 )
	ORTSBoilerEfficiency ( 5.0 0.80  160.0 0.40 )
	ORTSBurnRate ( 0.0 10.0  3842.9 376.7  9398.3 1005.0  13452.2 1507.0  17079.4 2009.0  20279.7 2511.0  23060.9 3014.0  25407.4 3516.0  27327.0 4018.0  28819.8 4520.0  29891.9 5023.0  30530.7 5525.0  30742.9 6027.0 ) 

	Comment ( "Cilindros" )

	NumCylinders ( 2 ) 
	CylinderStroke ( 25.98in ) 
	CylinderDiameter ( 23.62in ) 
	CylinderVolume ( 26.36 ) 
	CylinderEffectivity ( 1.45 ) 
	InjectorSizes ( 11mm 12mm ) 
	PrimingFactor ( 1 ) 
	ORTSCylinderEfficiencyRate ( 1 )	
	
	Comment ( "Combustión" )
	
	MaxFireMass ( 1205.4lb ) 
	IdealFireMass ( 753.4lb ) 
	MaxWaterMass ( 7180.9lb ) 
	SafetyValvesSteamUsage ( 16200lb/h ) 
	ShovelCoalMass ( 1lb ) 
	SmokeCombustion ( 1 )
	SteamFiremanMaxPossibleFiringRate ( 6027 ) 
	ORTSFuelCalorific ( 13000btu/lb )
	ORTSSteamFiremanMaxPossibleFiringRate ( 4500 ) 
 
	MaxTenderCoalMass ( 13228lb ) 
	MaxTenderWaterMass ( 44092lb ) 
	comment (0 for live steam, 1 for exhaust steam)
	InjectorTypes ( 0 1 ) 
	SuperHeater ( 1.32 ) 
	SteamSmokeUnitsPerPoundOfFuel ( 1 ) 
	SteamMaxSmokeUnitsReleaseRate ( 10 ) 
	MaxSteamHeatingPressure ( 80 ) 
	SafetyValvePressureDifference ( 5 ) 
	SteamGaugeGlassHeight ( 10.96 )
 
	BasicSteamUsage ( 600.0lb/h ) 
	BasicCoalUsage ( 376.7lb/h )
	
	comment ( min steam pressure, min water proportion, max water proportion  )
	InjectorLimits1 ( 50psi 0.6 1 ) 
	InjectorLimits2 ( 60psi 0 1 ) 
	CylinderCocksPowerEfficiency ( 0.8 ) 
	SteamCylinderCocksOperation ( Manual )
 
	RegulatorValveType ( Single_port ) 
	RegulatorMainValveExponent( 1 ) 

	SteamBlowerEffectExponent ( 0.9 ) 
	SteamBlowerEfficiencyExponent ( 1.1 ) 
	SteamBlowerMaxSteamUsageRate ( 500 ) 
	comment ( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect ( 0.15 )  
	SteamSmokeUnitsPerPoundOfFuel ( 6.3 )

	Comment ( "Frenos. Configurados de aire comprimido para ser compatibles con el material remolcado." )

	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 25.93 )
	AirBrakesCompressorRestartPressure( 95 )
	ORTSMainResChargingRate( 0.237 )
	ORTSBrakePipeChargingRate( 90 )
	TrainPipeLeakRate( 0.335 )
	ORTSBrakePipeTimeFactor( 0.002 )
	ORTSBrakeServiceTimeFactor( 0.02 )
	ORTSBrakeEmergencyTimeFactor( 0.1 )

	comment ( MSTS residual )

	AirBrakesAirCompressorPowerRating( 3.93 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 2 )
	AirBrakesHasLowPressureTest( 1 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	TrainBrakesControllerMaxSystemPressure( 70 )
	TrainBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 35 )
	TrainBrakesControllerFullServicePressureDrop( 26 )
	TrainBrakesControllerMinPressureReduction( 6 )

	comment ( MSTS residual )

	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 60 )

	EngineBrakesControllerMaxSystemPressure( 60 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	EngineBrakesControllerMaxApplicationRate( 2.667 )
	EngineBrakesControllerEmergencyApplicationRate( 7 )
	EngineBrakesControllerFullServicePressureDrop( 20 )
	EngineBrakesControllerMinPressureReduction( 6 )
	
	comment ( MSTS residual )

	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 60 )
	EngineBrakesControllerDirectControlExponent( 1 )

	comment ( Sistema de frenado )

	BrakesEngineBrakeType ( "Air_single_pipe"  )
	BrakesTrainBrakeType ( "Air_single_pipe" )
	BrakesEngineControllers( "Train, Independent" )	
 
	CabView ( "RN140SM.cvf" ) 
	HeadOut ( 1.7 3.4 -5.5 )
 
	EngineControllers ( 
		comment ( Engine controls )
		Regulator ( 0 1 0.025 0 
			NumNotches ( 0 
			) 
		) 
		Cutoff ( -0.75 0.75 0.01 0 
			NumNotches ( 0 
			) 
		) 
		Brake_Train ( 0 1 0.02 0.3 
			NumNotches ( 3 
				Notch ( 0 0 TrainBrakesControllerReleaseStart ) 
				Notch ( 0.3 0 TrainBrakesControllerRunningStart )
				Notch ( 0.5 0 TrainBrakesControllerSelfLapStart ) 
				Notch ( 0.6 1 TrainBrakesControllerApplyStart ) 
				Notch ( 0.9 0 TrainBrakesControllerEmergencyStart )
			) 
		)

		Brake_Engine ( 0 1 0.04 0.5
                NumNotches( 3
                    Notch(0   0 EngineBrakesControllerReleaseStart )
                    Notch(0.4 1 EngineBrakesControllerApplyStart )
		    Notch(0.8 0 EngineBrakesControllerEmergencyStart )
                )
            )            
 
		Brake_Hand ( 0 1 0.0125 0 
			NumNotches ( 0 
			) 
		) 
		FireDoor ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Sanding ( 0 1 0 ) 
		Blower ( 0 1 0.025 0.2 
			NumNotches ( 0 
			) 
		) 
		HeatingTap ( 0 1 0.025 0 
			NumNotches ( 0 
			) 
		) 
		Shovel ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		DampersFront ( 0 1 0.1 1 
			NumNotches ( 0 
			) 
		) 
		DampersBack ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Injector1Steam ( 0 1 0 ) 
		Injector2Steam ( 0 1 0 ) 
		Injector1Water ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		Injector2Water ( 0 1 0.1 0 
			NumNotches ( 0 
			) 
		) 
		CylinderCocks ( 0 1 1 ) 
		Whistle ( 0 1 0 ) 
		Waterscoop ( 0 1 0 ) 
		SmallEjectorOrCompressor ( 0 1 1 ) 
		HeadLights ( 0 1 0 ) 
	) 
	comment (fire temp, fire mass, water mass, boiler pressure,
		water level, tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )
	EngineVariables ( 850 753.4 5744.7 190.0 0 0 0 200 1 1 )
 
	Sound ( "RN140SMcab.sms" ) 
	Name ( "RN140-2505" ) 
	Description ( "Locomotora " ) 
	EngineOperatingProcedures ( "To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to increase the Regulator setting.\n"+  
	"4.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n"+
	"2. To hold the brakes at their current setting, lower the brake lever until it's in its middle (Neutral) position, by pressing the ; (SEMICOLON) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press  the ; (SEMICOLON) key to release the train brakes.\n"+
	"2. When the brakes are released, raise the brake lever until it's in its middle (Neutral) position, by pressing the ' (APOSTROPHE) key.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n\n"+
	"To operate the blower\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+ 
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2." ) 
) 