SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Renfe_Elos_R_Bauxita_F
	Type ( Freight )
	WagonShape ( FS_E507_2_105.s )
	Name ( "Renfe Elos Rojo Bauxita Cola" )
	Size ( 2.99664m 3.29336m 9.85m )
	FreightAnim ( Bauxite-3.s 1 1 )
	CentreOfGravity ( 0.0m 0.0m 0.0m )
	Mass ( 40t )
	InertiaTensor ( Box (2.99664m 3.29336m 9.65m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 20cm )
		)
		CouplingHasRigidConnection (1)
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 20cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

	Lights	(	2

		Light	(
			comment( R Rear red light )
			Type		( 0 )
			Conditions	(
				Service( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	2
				State	(
					Duration ( 1.4 )
					LightColour ( 00000000 )
					Position ( 0.91 1.43 -4.56 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				State	(
					Duration ( 0.04 )
					LightColour ( ffff0000 )
					Position ( 0.91 1.43 -4.56 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
		Light	(
			comment( L Rear red light )
			Type		( 0 )
			Conditions	(
				Service( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	2
				State	(
					Duration ( 1.7 )
					LightColour ( 00000000 )
					Position ( -0.91 1.43 -4.56 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				State	(
					Duration ( 0.04 )
					LightColour ( ffff0000 )
					Position ( -0.91 1.43 -4.56 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.4 )
				)
			)
		)
	)
    	
	BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 13.2kN )

	MaxHandbrakeForce( 35kN )
	EmergencyBrakeResMaxPressure( 70 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 25 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 18 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )

	Adheasion ( 1 1 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*40t )
	DerailBufferForce ( 800kN )
	WheelRadius ( 0.48m )
	NumWheels (	2 )
	Friction (
		366N/m/s			0		1mph		2.76N/m/s		1.8
		5.1N/rad/s		1		-1rad/s		0		1
	)

	Sound ( "GenFreightWag4.sms" )


)
