SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( Faccpps_RV_Lleno_F
	Name ( "Renfe Faccpps Rojo EpV Lleno cola" )
	Type ( Freight )
	Freightanim ( Lucescola.s 1 1 )
	WagonShape ( Faccpps_RV_Lleno.s )
	Size ( 3.10m 4.07m 12.08m )
	Mass ( "55t" )
	WheelRadius ( 47cm )
	CentreOfGravity ( 0m 1.0m 0m )
	InertiaTensor ( Box ( 3.10m 4.07m 12.08m  ) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.01m/s )
	)
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 7.5e6N/m 1e7N/m )
			Damping ( 1e6N/m/s 2e6N/m/s )
			Break ( 1.1e8N 5e8N )
			r0 ( 30cm 60cm )
		)
		CouplingHasRigidConnection ()
		Velocity ( 0.01m/s )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*23t )
	DerailBufferForce ( 350kN )
	NumWheels (	4 )
	Friction (
		489.5N/m/s		-0.1		1.7mph	3.589N/m/s		1.979
		5.1N/rad/s		1		-1rad/s		0		1
	)

Lights	(	2
			
		Light	(
			comment( Rear red light flashing dim )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	2
				State	(
					Duration ( 0.25 )
					LightColour ( eeff0000 )
					Position ( 0.87 1.6 -5.77 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
				State	(
					Duration ( 0.75 )
					LightColour ( 00000000 )
					Position ( 0.87 1.6 -5.77 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
		Light	(
			comment( Rear red light flashing bright )
			Type	 	( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	2
				State	(
					Duration ( 0.55 )
					LightColour ( eeff0000 )
					Position ( -0.87 1.6 -5.77 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
				State	(
					Duration ( 0.25 )
					LightColour ( 00000000 )
					Position ( -0.87 1.6 -5.77 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 1.0 )
				)
			)
		)
	)

	BrakeEquipmentType( "Handbrake, Graduated_release_Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 50kN )

	MaxHandbrakeForce( 5kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 1.24 )
	MaxReleaseRate( 0.8 )
	MaxApplicationRate( 0.8 )
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 7 )
	EmergencyResChargingRate( 30 )
	EmergencyBrakeResMaxPressure( 73 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 35 )

	Sound ( "..\\..\\SONIDOS_HIRES\\CISTERNAS\\CISTERNAS.sms" )
)
