SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RNX3B_BCh1LCi
	Type ( Freight )
	WagonShape ( RNX3B_08LC.s )
	Name ("Renfe X300 Balconcillo Bobinas de chapa metálicas de pie Luces cola inv")
	Freightanim ( X3FABOB1.s 1 1 )
	Size ( 3.28m 2.85m 10m )
	Mass ( 30.6t )
	WheelRadius ( 33in/2 )
	InertiaTensor ( Box (3.28m 2.85m 9.5m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 20cm )
		)
		Velocity ( 0.1m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			r0 ( 0m 1e9 )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*30.6t )
	DerailBufferForce ( 299.98kN )
	WheelRadius ( 0.448m )
	ORTSMaximumWheelFlangeAngle ( 70deg )
	ORTSWheelFlangeLength ( 1.0in )
	ORTSLengthCouplerFace ( 10m )
	ORTSLengthCarBody ( 9.5m )
	ORTSNumberAxles ( 2 )
	Friction (
		618.5N/m/s    -0.25    6.0mph    4.573N/m/s    1.701
		5.1N/rad/s		1		-1rad/s		0		1
	)

	BrakeEquipmentType( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 35.98kN )

	MaxHandbrakeForce( 12kN )
	NumberOfHandbrakeLeverSteps( 100 )

	TripleValveRatio( 2.5 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 25 )
	MaxAuxilaryChargingRate( 5 )
	EmergencyResCapacity( 7 )
	EmergencyResChargingRate( 5 )
	EmergencyBrakeResMaxPressure( 90 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )

  	Sound ( "FREIGHT.sms" )

	Lights	(	5

		Light	( 
			comment ( Luz trasera derecha roja )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 3 ) 
			) 
			FadeIn ( 0.5 ) 
			FadeOut ( 0.5 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( ffff0000 ) 
					Position ( 1.66 2.44 -4.46 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Luz trasera izquierda roja )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 3 ) 
			) 
			FadeIn ( 0.5 ) 
			FadeOut ( 0.5 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( ffff0000 ) 
					Position ( -1.66 2.44 -4.46 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Luz trasera derecha blanca )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 3 ) 
			) 
			FadeIn ( 0.5 ) 
			FadeOut ( 0.5 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffdf90 ) 
					Position ( 1.66 2.44 -4.21 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Luz trasera izquierda blanca )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 3 ) 
			) 
			FadeIn ( 0.5 ) 
			FadeOut ( 0.5 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( d8ffdf90 ) 
					Position ( -1.66 2.44 -4.21 ) 
					Azimuth ( 0 0 0 ) 
					Transition ( 0 ) 
					Radius ( 0.4 ) 
					) 
				) 
			) 
		Light	( 
			comment ( Luz trasera baja roja )
			Type ( 0 ) 
			Conditions ( 
				Service ( 2 ) 
				Unit ( 3 ) 
			) 
			FadeIn ( 0.5 ) 
			FadeOut ( 0.5 ) 
			Cycle ( 0 ) 
			States ( 1 
				State ( 
					Duration ( 0.0 ) 
					LightColour ( ffff0000 ) 
					Position ( -0.50 1.38 -4.63 ) 
					Azimuth ( 180 180 180 ) 
					Transition ( 0 ) 
					Radius ( 0.8 ) 
					) 
				) 
			)
		)

)