SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RNSS301
	Type ( Carriage )
	WagonShape ( RNSS301.s )
	FreightAnim ( SSint.s 1 1 )	
	Size ( 3.23m 4.09m 18.55m )
	CentreOfGravity ( 0.0m 0.0m 0.0m )
	Mass ( 32t )
	InertiaTensor ( Box (3.23m 4.09m 18.05m) )
	
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s)
			Break ( 5.1e7N 5.1e7N )
			r0 ( 10cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.2m/s )
	)
	Buffers (
		Spring (
			Stiffness ( 9.8e5N/m 9.8e5N/m )
			Damping ( 1.7e6N/m/s 1.7e6N/m/s )
			r0 ( 20cm 30cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	BrakeEquipmentType ( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
	BrakeSystemType ( "Air_single_pipe" )
	MaxBrakeForce( 37.63kN )

	MaxHandbrakeForce( 12.54kN )
	EmergencyBrakeResMaxPressure( 70 )
	TripleValveRatio( 2.5 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 25 )
	EmergencyResCapacity( 14 )
	EmergencyResChargingRate( 18 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*32t )
	DerailBufferForce ( 800kN )
	WheelRadius ( 0.4825m )
	ORTSLengthCarBody ( 20.1m )
	ORTSLengthCouplerFace ( 21m )
	ORTSNumberBogies ( 2 )
	ORTSNumberAxles ( 4 )
	ORTSWheelFlangeLength ( 2.54mm )
	ORTSMaximumWheelFlangeAngle ( 70deg )
	Friction (
		945.7N/m/s    -0.25    6.0mph    3.043N/m/s    1.710
		5.1N/rad/s		1		-1rad/s		0		1
	)
	
	
	        comment ( === Vistas interiores con Mayúsculas + 5 === )

    Inside (
	   PassengerCabinFile     ( "SSint.s" )
	   PassengerCabinHeadPos ( 1.15 2.45 8.5 )
	   RotationLimit ( 360 360 360 )
	   StartDirection ( 0 -160 0 )
	   Sound ( "vapor4e_pas.sms" )
	)
	Inside (
	   PassengerCabinFile     ( "SSint.s" )
	   PassengerCabinHeadPos ( -1.35 2.45 -1.6 )
	   RotationLimit ( 360 360 360 )
	   StartDirection ( 0 25 0 )
	   Sound ( "vapor4e_pas.sms" )
	)
	
	
	                     comment ( === Luces === )
	
    Lights ( 15
    Light (
    comment( cola reducido bajo rojo )
    Type  ( 0 )
    Conditions (
       Headlight ( 2 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
        Duration ( 0.0 )
        LightColour ( D0ff0000 )
        Position ( 0.79 1.55 -8.95  )
        Azimuth ( -180 -180 -180 )
        Transition ( 0 )
        Radius ( 1 )
      )
     )
    )
   Light (
   comment( cola reducido derecha rojo )
   Type  ( 0 )
   Conditions (
    Headlight ( 2 )
    Unit ( 3 )
   )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle  ( 0 )
   States ( 1
    State (
        Duration ( 0.0 )
        LightColour ( 80ff0000 )
        Position ( 1.52 2.95 -8.97 )
        Azimuth ( -180 -180 -180 )
        Transition ( 0 )
        Radius ( 1 )
      )
     )
    )
    Light (
    comment( cola reducido izquierda rojo )
    Type  ( 0 )
    Conditions (
       Headlight ( 2 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
         Duration ( 0.0 )
         LightColour ( 80ff0000 )
         Position ( -1.52 2.95 -8.97 )
         Azimuth ( -180 -180 -180 )
         Transition ( 0 )
         Radius ( 1 )
       )
      )
    )
    Light (
    comment( cola reducido derecha blanco )
    Type  ( 0 )
    Conditions (
       Headlight ( 2 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
       Duration ( 0.0 )
       LightColour ( cdffffb5 )
        Position ( 1.52 2.95 -8.70 )
        Azimuth ( 0 0 0 )
        Transition ( 0 )
        Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola reducido izquierda blanco )
    Type  ( 0 )
    Conditions (
       Headlight ( 2 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
       Duration ( 0.0 )
       LightColour ( cdffffb5 )
       Position ( -1.52 2.95 -8.70 )
       Azimuth ( 0 0 0 )
       Transition ( 0 )
       Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola pleno bajo rojo )
    Type  ( 0 )
    Conditions (
       Headlight ( 3 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
        Duration ( 0.0 )
        LightColour ( D0ff0000 )
        Position ( 0.79 1.55 -8.95 )
        Azimuth ( -180 -180 -180 )
        Transition ( 0 )
        Radius ( 1 )
       )
      )
    )
    Light (
    comment( cola pleno derecha rojo )
    Type  ( 0 )
    Conditions (
       Headlight ( 3 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
       Duration ( 0.0 )
       LightColour ( 80ff0000 )
       Position ( 1.52 2.95 -8.97 )
       Azimuth ( -180 -180 -180 )
       Transition ( 0 )
       Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola pleno izquierda rojo )
    Type  ( 0 )
    Conditions (
       Headlight ( 3 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
         Duration ( 0.0 )
         LightColour ( 80ff0000 )
         Position ( -1.52 2.95 -8.97 )
         Azimuth ( -180 -180 -180 )
         Transition ( 0 )
         Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola pleno derecha blanco )
    Type  ( 0 )
    Conditions (
       Headlight ( 3 )
       Unit ( 3 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
       Duration ( 0.0 )
       LightColour ( cdffffb5 )
       Position ( 1.52 2.95 -8.70 )
       Azimuth ( 0 0 0 )
       Transition ( 0 )
       Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola pleno izquierda blanco )
    Type  ( 0 )
    Conditions (
       Headlight ( 3 )
       Unit ( 3 )
     )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
        Duration ( 0.0 )
        LightColour ( cdffffb5 )
        Position ( -1.52 2.95 -8.70 )
        Azimuth ( 0 0 0 )
        Transition ( 0 )
        Radius ( 0.5 )
       )
      )
    )
    Light (
    comment( cola AI bajo rojo )
    Type  ( 0 )
    Conditions (
       Control ( 1 )
       Unit ( 3 )
       Service ( 2 )
       TimeOfDay ( 0 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
       Duration ( 0.0 )
       LightColour ( D0ff0000 )
       Position ( 0.79 1.55 -8.95  )
       Azimuth ( -180 -180 -180 )
       Transition ( 0 )
       Radius ( 1 )
       )
      )
    )
    Light (
    comment( cola AI derecha rojo )
    Type  ( 0 )
    Conditions (
       Control ( 1 )
       Unit ( 3 )
       Service ( 2 )
       TimeOfDay ( 0 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
         Duration ( 0.0 )
         LightColour ( 80ff0000 )
         Position ( 1.52 2.95 -8.97 )
         Azimuth ( -180 -180 -180 )
         Transition ( 0 )
         Radius ( 1 )
        )
       )
    )
    Light (
    comment( cola AI izquierda rojo )
    Type  ( 0 )
    Conditions (
       Control ( 1 )
       Unit ( 3 )
       Service ( 2 )
       TimeOfDay ( 0 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
         Duration ( 0.0 )
         LightColour ( 80ff0000 )
         Position ( -1.52 2.95 -8.97 )
         Azimuth ( -180 -180 -180 )
         Transition ( 0 )
         Radius ( 1 )
        )
       )
    )
    Light (
    comment( cola AI derecha blanco )
    Type  ( 0 )
    Conditions (
       Control ( 1 )
       Unit ( 3 )
       Service ( 2 )
       TimeOfDay ( 0 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
          Duration ( 0.0 )
          LightColour ( cdffffb5 )
          Position ( 1.52 2.95 -8.70 )
          Azimuth ( 0 0 0 )
          Transition ( 0 )
          Radius ( 0.5 )
         )
        )
    )
    Light (
    comment( cola AI izquierda blanco )
    Type  ( 0 )
    Conditions (
       Control ( 1 )
       Unit ( 3 )
       Service ( 2 )
       TimeOfDay ( 0 )
    )
    FadeIn ( 0.5 )
    FadeOut ( 0.5 )
    Cycle  ( 0 )
    States ( 1
       State (
         Duration ( 0.0 )
         LightColour ( cdffffb5 )
         Position ( -1.52 2.95 -8.70 )
         Azimuth ( 0 0 0 )
         Transition ( 0 )
         Radius ( 0.5 )
            )
          )
        )
    ) 
 
 
 
                     comment ( === Efectos especiales === )
					 

    ORTSWagonSpecialType ( Heated )
	
	Effects (
    SpecialEffects ( 	       				
			comment ( === Vapor mangueras calefacción === )
			HeatingHoseFX(
                0.0 0.25 8.9
                0 1 0
                0.05
            )
			comment ( === Vapor calefacción === )
			HeatingHoseFX(
                -1.1 0.7 1.4
                -0.6 -1 0.5
                0.15
            )
			comment ( === Vapor calefacción === )
			HeatingHoseFX(
                -1.1 0.7 1.3
                -0.6 -1 0.5
                0.15
            )
			comment ( === Vapor calefacción === )
			HeatingHoseFX(
                -1.1 0.7 -1.3
                -0.6 -1 0.5
                0.15
            )
			comment ( === Vapor calefacción === )
			HeatingHoseFX(
                -1.1 0.7 -1.4
                -0.6 -1 0.5
                0.15
            )					
		)
	)
	
	
	Comment ( **************************** Calefacción de vapor del coche ****************************
          Punto de ajuste de la temperatura de la cabina, dimensiones de la tubería de calefacción, etc.
          ********************************************************************************* )

    ORTSHeatingCompartmentTemperatureSet ( 68degF )
    ORTSHeatingCompartmentPipeAreaFactor ( 1.0 )
    ORTSHeatingWindowDeratingFactor ( 0.25 )
    ORTSHeatingTrainPipeOuterDiameter (  2.875in  )
    ORTSHeatingTrainPipeInnerDiameter ( 2.07in )
    ORTSHeatingConnectingHoseOuterDiameter ( 2.05in )
    ORTSHeatingConnectingHoseInnerDiameter ( 1.5in )
 
 
 
    Sound ( "vapor4e_wag.sms" )


    )
