SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RNDGDC3203
	Type ( Carriage )
	WagonShape ( RNDGDC3203.s )
	
	Size ( 3.19m 4.33m 20.55m )
	CentreOfGravity ( 0.0m 0.0m 0.0m )
	Mass ( 32t )
	InertiaTensor ( Box (3.19m 4.33m 20.1m) )
	
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 1e6N/m/s )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 0cm 20cm )
		)
		CouplingHasRigidConnection ( 1 )
		Velocity ( 0.2m/s )
	)
	
	Buffers (
		Spring (
			Stiffness ( 9.8e5N/m 9.8e5N/m )
			Damping ( 1.7e6N/m/s 1.7e6N/m/s )
			r0 ( 10cm 20cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)

		
		       comment ( Vistas interiores con Mayúsculas + 5 sucesívamente )
	
	Inside (
		PassengerCabinFile ( RNDGDC3203.s )
		PassengerCabinHeadPos ( 1 2.7 -0.9 )
        RotationLimit ( 0 0 0 )
		StartDirection ( 0 -10 0 )
		Sound ( "Vagon_int.sms" )
	)
	
	Inside (
		PassengerCabinFile ( RNDGDC3203.s )
		PassengerCabinHeadPos ( 1.15 2.7 1.75 )
        RotationLimit ( 0 0 0 )
		StartDirection ( 7 -90 0 )
		Sound ( "Vagon_int.sms" )
	) 
	
	Inside (
		PassengerCabinFile ( RNDGDC3203.s )
		PassengerCabinHeadPos ( 1 2.7 14.3 )
        RotationLimit ( 0 0 0 )
		StartDirection ( 0 -20 0 )
		Sound ( "Vagon_int.sms" )
	)
	
	
    Lights	(	11

comment(               luces traseras             )

		Light	(
			comment( cola lfm pleno derecha )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.99 2.940 -10.11  )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lfm pleno izquierda )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.99 2.940 -10.11  )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lfm pleno inferior )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.99 1.39 -10.13 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)

comment(               luces delanteras             )

		Light	(
			comment( cola lofm pleno derecha )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.99 2.940 10.11  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lofm pleno izquierda )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.99 2.940 10.11  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lofm pleno inferior )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 4 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.99 1.39 10.13  )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)

comment(               luces delanteras IA             )

		Light	(
			comment( cola lofm pleno derecha )
			Type		( 0 )
			Conditions	(
				Control ( 1 )
				Unit ( 3 )
				Service ( 2 )
				TimeOfDay ( 0 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.99 2.940 10.11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lofm pleno izquierda )
			Type		( 0 )
			Conditions	(
				Control ( 1 )
				Unit ( 3 )
				Service ( 2 )
				TimeOfDay ( 0 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.99 2.940 10.11 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( cola lofm pleno inferior )
			Type		( 0 )
			Conditions	(
				Control ( 1 )
				Unit ( 3 )
				Service ( 2 )
				TimeOfDay ( 0 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.99 1.39 10.13 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.9 )
				)
			)
		)	

		Light	(
			comment( alarma lfm derecha )
			Type		( 0 )
			Conditions	(
				Unit ( 1 )
				Penalty ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff6a00 )
					Position ( 1.43 3.00 -9.88 )
					Azimuth ( 90 90 90 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
		Light	(
			comment( alarma lfm izquierda )
			Type		( 0 )
			Conditions	(
				Unit ( 1 )
				Penalty ( 2 )
			)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle		( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff6a00 )
					Position ( -1.43 3.00 -9.88 )
					Azimuth ( -90 -90 -90 )
					Transition ( 0 )
					Radius ( 0.45 )
				)
			)
		)
	)		
	
	BrakeEquipmentType ( "Handbrake, Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
    BrakeSystemType ( "Air_single_pipe" )
    MaxBrakeForce( 37.63kN )

    MaxHandbrakeForce( 12.54kN )
    NumberOfHandbrakeLeverSteps( 100 )
    TripleValveRatio( 2.5 )
    MaxReleaseRate( 15 )
    MaxApplicationRate( 25 )
    MaxAuxilaryChargingRate( 5 )
    EmergencyResCapacity( 7 )
    EmergencyResChargingRate( 5 )
    EmergencyBrakeResMaxPressure( 90 )
    BrakeCylinderPressureForMaxBrakeBrakeForce( 50 )

	Adheasion ( 0.2 0.4 2 0 )
	DerailRailHeight ( 10cm )
	DerailRailForce ( 2.5*32t )
	DerailBufferForce ( 800kN )
	WheelRadius ( 0.4825m )
	NumWheels (	4 )
	Friction (
		945.7N/m/s    -0.25    6.0mph    2.690N/m/s    1.748
		5.1N/rad/s		1		-1rad/s		0		1
	)

	Sound ( "genpasswagmodern.sms" )
)
