SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN1103

    Type ( Engine )
    WagonShape ( RN1103.s )
  
    comment(--- Características generales ---)
    Mass ( 67.5t )
    Size  ( 3.18m 5.38m 12.58m )
    CentreOfGravity ( 0m 2.25m 0m )
    InertiaTensor ( Box (3.18m 5.38m 12.08m) )

    comment(---Rodadura---)
    WheelRadius ( 0.635m )
    NumWheels ( 4 )
    Adheasion ( 0.2 0.4 2 0 )

    Friction (
        943.0N/m/s    -0.10    1.6mph    10.672N/m/s    1.847
        5.1N/rad/s       1         -1rad/s      0               1
    )
	
    comment(---Descarrilamiento---)
    DerailRailHeight ( 10cm )
    DerailRailForce ( 2.5*67.5t )
    DerailBufferForce ( 800kN )

    comment(---Enganche---)
    Coupling (
        Type ( Automatic )
        Spring (
            Stiffness ( 1e6N/m 5e6N/m )
            Damping ( 1e6N/m/s 1e6N/m/s )
            Break ( 5.1e7N 5.1e7N )
            r0 ( 10cm 20cm )
        )
        CouplingHasRigidConnection ( 0 )
        Velocity ( 0.1m/s )
    )

    Buffers (
        Spring (
            Stiffness ( 1e6N/m 5e6N/m )
            Damping ( 1e6N/m/s 1e6N/m/s )
            r0 ( 0m 1e9 )
        )
        Centre ( 0.5 )
        Radius ( 1 )
        Angle ( 0.5deg )
    )
    
	Comment (---Vistas interiores---)
	
	    Inside (
            PassengerCabinFile ( RN1103.s )
            PassengerCabinHeadPos ( 1.1 2.9 -1 )
            RotationLimit ( 90 90 90 )
            StartDirection ( 0 0 0 )
            Sound ( "Brillcab.sms" )
	)
		Inside (
            PassengerCabinFile ( RN1103.s )
            PassengerCabinHeadPos ( 1.1 2.9 1 )
            RotationLimit ( 90 90 90 )
            StartDirection ( 0 180 0 )
            Sound ( "Brillcab.sms" )
	)
	    Inside (
            PassengerCabinFile ( RN1103.s )
            PassengerCabinHeadPos ( -1.5 2.2 -5.3 )
            RotationLimit ( 90 90 90 )
            StartDirection ( 30 135 0 )
            Sound ( "Brilleng.sms" )
	)
	
    comment(---Frenado---)
	
    BrakeEquipmentType( "graduated_release_triple_valve , Auxilary_reservoir, Emergency_brake_reservoir" )
    BrakeSystemType ( "Air_single_pipe" )
    MaxBrakeForce ( 64.125kN )
    EmergencyBrakeResMaxPressure( 110 )
    TripleValveRatio( 2.5 )
    MaxReleaseRate( 10 )
    MaxApplicationRate( 5 )
    MaxAuxilaryChargingRate( 5 )
    EmergencyResCapacity( 7 )
    EmergencyResChargingRate( 5 )
    EmergencyBrakeResMaxPressure( 140 )
    BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

    BrakeDistributorFullServicePressure( 82 )
    BrakeDistributorMaxAuxilaryResPressure( 110 )
    BrakeDistributorEmergencyResPressure( 110 )
    BrakeDistributorReleaseRate( 10 )
    BrakeDistributorApplicationRate( 15 )
    BrakeDistributorTrainPipeControlRatio( 2.03 )
    BrakeDistributorNormalFullReleasePressure( 110 )
	Brakepipevolume ( 0.5 )


    comment(---Luces---)

	Lights	( 16

           Light	(
			comment( Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0.0 3.94 6 )
					Transition ( 0 )
					Radius ( 100.0 )
					Angle ( 10.0 )
					)
				)
			)		
           Light	(
			comment( Sphere of light )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0.0 3.94 6 )
					Transition ( 0 )
					Radius ( 250.0 )
					Angle ( 15.0 )
					)
				)
			)
           Light	(
			comment( Foco central del Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0 3.94 5.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
           Light	(
			comment( Foco central del Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0 3.94 5.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
           Light	(
			comment( Delantero inf derecho )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 1.10 1.84 5.92 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
           Light	(
			comment( Delantero inf izquierdo )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( -1.10 1.84 5.92 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
          Light		(
			comment( Delantero Sup derecho )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.26 3.40 5.35 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
          Light		(
			comment( Delantero Sup izquierda )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.26 3.40 5.35 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)

comment(     luces reversibles    )

           Light	(
			comment( Foco central del Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0 3.94 -5.76 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.4 )
					)
				)
			)
           Light	(
			comment( Foco central del Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0 3.94 -5.76 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
           Light	(
			comment( Delantero inf derecho )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 1.10 1.84 -5.92 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
           Light	(
			comment( Delantero inf izquierdo )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( -1.10 1.84 -5.92 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
          Light		(
			comment( Delantero Sup derecho )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( 1.26 3.40 -5.35 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
          Light		(
			comment( Delantero Sup izquierda )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( ffff0000 )
					Position ( -1.26 3.40 -5.35 )
					Azimuth ( 180 180 180 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)

comment(      luces IA        )

           Light	(
			comment( Foco central del Bright )
			Type		( 0 )
			Conditions	(
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 )
				TimeOfDay ( 0 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( d8ffdf90 )
					Position ( 0 3.94 5.76 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					)
				)
			)
	      Light	(
			comment( Pantograph flash )
			Type		( 0 )
			Conditions	(
				Service ( 2 )
				Unit ( 0 )
				)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.37 -3.33 )
					Azimuth ( 0.0 -180.0 180.0 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)											
		)

    Sound ( "brilleng.sms" )
		
)

Engine ( RN1103

    comment(---Características generales ---)
    Name ( "RN1103" )
    Wagon ( RN1103 )

    Type ( Electric )
    
    MaxVelocity ( 70kmh )
    WheelRadius ( 0.635m )
    MaxPower ( 824kW )
    MaxForce ( 147.1kN )
    MaxContinuousForce ( 117.68kN )
	ORTSSpeedOfMaxContinuousForce (3kmh )

    MaxCurrent ( 2000A )
    NumWheels ( 4 )
    Sanding ( 1e9mph )

    AntiSlip (1)
    MaxSandingTime ( 1800s )

	Comment (---Frenos sección motriz---)
	
    AirBrakesAirCompressorPowerRating( 2 )
	AirBrakesMainMinResAirPressure( 50 )
	AirBrakesMainMaxAirPressure( 100 )
	AirBrakesMainResVolume( 8 )
	AirBrakesAirCompressorWattage( 10000 )
	AirBrakesCompressorRestartPressure( 120 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 1.5 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerMinPressureReduction ( 7 )
	EngineBrakesControllerMaxApplicationRate ( 30 )
	EngineBrakesControllerMaxReleaseRate ( 40 )
	EngineBrakesControllerMinSystemPressure ( 0 )
	EngineBrakesControllerMaxSystemPressure ( 110 )
    EngineBrakesControllerEmergencyApplicationRate ( 50 )
	EngineBrakesControllerEmergencyBrakeTimePenalty ( 120 )
	EngineBrakesControllerFullServicePressureDrop ( 50 )
	EngineBrakesControllerHasProportionalBrake ( 1 )
	EngineBrakesControllerDirectControlExponent ( 1 )
    EngineBrakesProportionalBrakeLag( 0.1 )
	EngineBrakeHasEmergencyStopButton ( 0 )
	
	MainResChargingRate ( 0.4 )
	EngineBrakeReleaseRate ( 12.5 )
	EngineBrakeApplicationRate ( 12.5 )
	BrakePipeChargingRate ( 21 )
	BrakeServiceTimeFactor ( 1.009 )
	BrakeEmergencyTimeFactor ( 0.1 )
	BrakePipeTimeFactor ( 0.003 )
               
	TrainBrakesControllerMinPressureReduction ( 6 )
	TrainBrakesControllerMaxApplicationRate ( 2 )
	TrainBrakesControllerMaxReleaseRate ( 2 )
	TrainBrakesControllerMinSystemPressure ( 0 )
	TrainBrakesControllerMaxSystemPressure ( 110 )
	TrainBrakesControllerMaxQuickReleaseRate ( 80 )
    TrainBrakesControllerEmergencyApplicationRate ( 50 )
	TrainBrakesControllerEmergencyBrakeTimePenalty ( 120 )
	TrainBrakesControllerFullServicePressureDrop ( 50 )
	TrainBrakesControllerDirectControlExponent ( 1 )
	TrainPipeLeakRate ( 5 )

	DynamicBrakesMinUsableSpeed( 4 )
	DynamicBrakesMaximumEffectiveSpeed( 23 )
	DynamicBrakesMaximumForce( 90kN )
	DynamicBrakesResistorCurrentLimit ( 3300A )
	DynamicBrakesCutInSpeed( 5 )
	DynamicBrakesMaxAirBrakePressure ( 50 )
	DynamicBrakesFadingSpeed( 17 )
	DynamicBrakesDelayTimeBeforeEngaging ( 8 )
	DynamicBrakesMaximumSpeedForFadeOut ( 80 )
	DynamicBrakesEffectAtMaximumFadeOut( 0.34 )
	DynamicBrakesHigherSpeedCurveExponent( 1.2 )
	DynamicBrakesLowerSpeedCurveExponent( 0.9 )
	DynamicBrakesNumberOfControllerNotches( 13 )
	DynamicBrakeHasAutoBailOff ( 0 )

      BrakesEngineBrakeType( "Air_single_pipe"  )
      BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Independent, Train, Dynamic" )

    CabView ( "RN1101.cvf" )
    HeadOut ( 1.6 3 2.9 )

    Sound ( "brillcab.sms" )

    comment(---Monitores---)
    EmergencyStopMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 0 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 0 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 1 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
    )

    AWSMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 7 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 0 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 0 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
    )

    VigilanceMonitor(
        MonitoringDeviceMonitorTimeLimit ( 60 )
        MonitoringDeviceAlarmTimeLimit ( 55 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 1 )
        MonitoringDeviceAppliesEmergencyBrake ( 0 )
        MonitoringDeviceAppliesCutsPower ( 0 )
        MonitoringDeviceAppliesShutsDownEngine ( 1 )
        MonitoringDeviceResetOnZeroSpeed ( 1 )
    )

    OverspeedMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 0 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 150 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 1 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 1 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
        MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
        MonitoringDeviceTriggerOnTrackOverspeedMargin ( 10 )
        MonitoringDeviceResetOnZeroSpeed ( 1 )
        MonitoringDeviceResetOnResetButton ( 0 )
    )

    comment(---Controles---)

    EngineControllers (
            Throttle ( 0 1 0.025 0
                NumNotches ( 12 )
				Notch ( 0 0 0 )
				Notch ( 0.05 0)
				Notch ( 0.10 0)
                Notch ( 0.20 0 )
                Notch ( 0.30 0 )
                Notch ( 0.35 0 )
                Notch ( 0.45 0 )
                Notch ( 0.60 0 )
                Notch ( 0.75 0 )
				Notch ( 0.85 0 )
				Notch ( 0.95 0)
                Notch ( 1 0 )
    			 )
	Brake_Train ( 0 1 0.02 0.4
                NumNotches ( 9
                    Notch ( 0 0 TrainBrakesControllerReleaseStart )
					Notch ( 0.10 0 )
                    Notch ( 0.25 0 TrainBrakesControllerHoldLappedStart )
                    Notch ( 0.35 0 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                    Notch ( 0.55 0 TrainBrakesControllerSuppressionStart )
                    Notch ( 0.75 0 TrainBrakesControllerContinuousServiceStart )
                    Notch ( 0.85 0 TrainBrakesControllerEmergencyStart )
					Notch ( 0.95 0 )
					Notch ( 1 0 )
                )
            )
             Brake_Engine ( 0 1 0.04 0 
                NumNotches ( 9
                    Notch ( 0 0 )
                    Notch ( 0.10 0 )
					Notch ( 0.20 0 )
					Notch ( 0.35 0 )
                    Notch ( 0.45 0 )
                    Notch ( 0.65 0 )
                    Notch ( 0.85 0 )
                    Notch ( 0.95 0 )
					Notch ( 1 0 )
                )
       	  )
            Brake_Dynamic ( 0 1 0.04 0 
                	NumNotches ( 13
                    Notch ( 0  0 )
                    Notch ( 0.05 0 )                  
                    Notch ( 0.10 0 )         
                    Notch ( 0.15 0 )
					Notch ( 0.20 0 )			
					Notch ( 0.25 0 )
					Notch ( 0.30 0 )
					Notch ( 0.35 0 )
					Notch ( 0.45 0 )
					Notch ( 0.65 0 )
					Notch ( 0.85 0 )
					Notch ( 0.95 0 )
					Notch ( 1 0 )
                )
            )
		Combined_Control( 0 1 0.1 0.5 throttle dynamic )
            DirControl ( -1 0 1 1 )
            BellToggle( 0 1 0 )
            Sanding ( 0 1 0 )
            Horn ( 0 1 0 )
            Wipers ( 0 1 0 )
            PantographToggle1 ( 0 1 0 )
            EmergencyStopResetToggle( 0 1 0 )
            EmergencyStopToggle( 0 1 0 )
            Vigilance ( 0 1 0 )
            Headlights ( 0 0.25 1 0 )
	)
    EngineVariables ( 5300 )

   Name ( "RN1103 282-003 época IV" )
      Description (
  "Constructores partes mecánicas: Babcock & Wilcox y General Electric \n"+
  "Constructores partes eléctricas: Westinghouse \n"+
  "Años de puesta en servicio: 1932 \n"+
  "Tensión:  1500 V. en C.C. \n"+
  "Disposición de ejes:  Co'Co' \n"+
  "Potencia nominal:  1.110 CV, 1.215 CV en régimen unihorario \n"+
  "Peso en servicio:  67.5 T \n"+
  "Esfuerzo tractor:  12000 kgs \n"+
  "Velocidad máxima  70 kmh \n"+
  "Número de motores:  4 \n"+

        )
     )
