SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( RN060-4008
	Type ( Engine )
	WagonShape ( RN060-4008.s )
	
	Size  ( 3.283m 4.139m 11.6m )
	CentreOfGravity ( 0.0m 2.16445m 0.0m )
	Centre ( 0m 0m 0m)
	Mass ( 73.13t )
	InertiaTensor ( Box(3.283m 4.139m 11.3m) )
	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e6N/m 1e6N/m )
			Break ( 5.1e7N 5.1e7N )
			r0 ( 20cm 40cm )
		)
		Velocity   ( 0.1m7s )	
	)
	Buffers (
		Spring (
		      Stiffness ( 1e6N/m 2e6N/m )
			Damping ( 1e6N/m 1e6N/m )
			r0 ( 20cm 40cm )
		)
		Centre ( 0.5 )
		Radius ( 1 )
		Angle ( 0.5deg )
	)
	 
	Adheasion ( 0.30 0.76 1.58 0 )
	DerailRailHeight ( 4cm )
	DerailRailForce ( 2.5*73.13t )
	DerailBufferForce ( 400kN )
	WheelRadius ( 0.4825m )
	NumWheels ( 6 )

	Comment ("Fórmula de F-calc Joe Realmuto")

	Friction ( 
		1207.38N/m/s  -0.10  1.6mph 8.171N/m/s  1.798
		5.1N/rad/s 1 -1rad/s 0 1
	)

	BrakeEquipmentType( "Triple_valve, Auxilary_reservoir, Handbrake" )
	BrakeSystemType( "Air_single_pipe" )
	MaxBrakeForce( 100.4kN )
	MaxHandbrakeForce( 50kN )
	NumberOfHandbrakeLeverSteps( 100 )
	MaxReleaseRate( 15 )
	MaxApplicationRate( 15 )
	MaxAuxilaryChargingRate( 15 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )        

	Lights ( 10

  		Light (
   			comment( Esfera luz frontal)
   			Type ( 1 )
   			Conditions(
    				Headlight ( 3 )
    				Unit ( 2 )
    				)
   			Cycle ( 0 )
   			FadeIn ( 0.5 )
   			FadeOut ( 0.5 )
   			States ( 1
    				State (
     					Duration ( 0.0 )
     					LightColour ( d8ffdf90 )
    					Position ( 0.0 3.562 4.164 )
     					Transition ( 0 )
     					Radius ( 200.0 )
     					Angle ( 15.0 )
     					)
    				)
  			)
		Light ( 
   			comment( Foco principal )
   			Type ( 0 )
   			Conditions (
    				Headlight ( 3 )
    				Unit ( 2 )
    				)
   			FadeIn ( 0.5 )
   			FadeOut ( 0.5 )
   			Cycle ( 0 )
   			States ( 1
    				State (
     					Duration ( 0.0 )
     					LightColour ( d8ffdf90 )
     					Position ( 0.0 3.562 4.164 )
     					Azimuth ( 0.0 0.0 5.0 )
     					Transition ( 0 )
     					Radius ( 0.7 )
     					)
    				)
   			)
		
		Light	(	
			comment( Lateral Foco Ppal derecha )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 90ffffb5 )
					Position ( -0.098 3.565 3.823)
					Azimuth (  -90.0 -90.0 -90.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		
		Light	(	
			comment( Lateral Foco Ppal izquierda )
			Type( 0 )
			Conditions (
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( 90ffffb5 )
					Position ( 0.098 3.565 3.823)
					Azimuth (  90.0 90.0 90.0 )
					Transition ( 0 )
					Radius ( 0.3 )
					)
				)
			)
		
		Light	(	
			comment( Luz posición central )
			Type( 0 )
			Conditions (
				Service ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			Cycle	( 0 )
			States	( 1
				State	(
					Duration ( 0.0 )
					LightColour ( b0ffffb5 )
					Position ( -0.30 3.417 3.876 )
					Azimuth ( 0.0 0.0 5.0 )
					Transition ( 0 )
					Radius ( 0.35 )
					)
				)
			)
		
		Light (
   			comment( Luz posición Dcha )
   			Type ( 0 )
   			Conditions (
    				Service ( 2 )
    				Unit ( 2 )
    				)
   			FadeIn ( 0.5 )
   			FadeOut ( 0.5 )
   			Cycle ( 0 )
   			States ( 1
    				State (
     					Duration ( 0.0 )
     					LightColour ( cdffff85 )
     					Position ( 1.002 1.931 4.83 )
     					Azimuth ( 0.0 -5.0 5.0 )
     					Transition ( 0 )
     					Radius ( 0.5 )
     					)
    				)
   			)
		Light (
   			comment( Luz posición izqda )
   			Type ( 0 )
   			Conditions (
    				Service ( 2 )
    				Unit ( 2 )
    				)
   			FadeIn ( 0.5 )
   			FadeOut ( 0.5 )
   			Cycle ( 0 )
   			States ( 1
    				State (
     					Duration ( 0.0 )
     					LightColour ( cdffff85 )
     					Position ( -1.002 1.931 4.83 )
     					Azimuth ( 0.0 -5.0 5.0 )
     					Transition ( 0 )
     					Radius ( 0.5 )
     					)
    				)
   			)

		Light ( 
   			comment( Foco Ppal IA )
   			Type ( 0 )
   			Conditions (
				Control ( 1 )
				Unit ( 2 )
				Service ( 2 )
				TimeOfDay ( 0 )
    				)
   			FadeIn ( 0.5 )
   			FadeOut ( 0.5 )
   			Cycle ( 0 )
   			States ( 1
    				State (
     					Duration ( 0.0 )
     					LightColour ( d8ffdf90 )
     					Position ( 0.0 3.562 4.164 )
     					Azimuth ( 0.0 0.0 5.0 )
     					Transition ( 0 )
     					Radius ( 0.7 )
     					)
    				)
   			)

		Light (
   			comment( Reflejo hogar Dcha )
   			Type ( 0 )
   			Conditions (
    				Headlight ( 0 )
    				Unit ( 0 )
    				)
   			FadeIn ( 0.1 )
   			FadeOut ( 0.1 )
   			Cycle ( 0 )
   			States ( 4
    				State (
     					Duration ( 0.1 )
     					LightColour ( 40fff080 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  -90.0 -90.0 -90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				State (
     					Duration ( 0.1 )
     					LightColour ( 00000000 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  -90.0 -90.0 -90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				State (
     					Duration ( 0.1 )
     					LightColour ( 40ffc080 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  -90.0 -90.0 -90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				State (
     					Duration ( 0.1 )
     					LightColour ( 20807040 )
    	 				Position ( 0.0 0.313 -2.506 )
     					Azimuth (  -90.0 -90.0 -90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				)
   			)
		Light (
   			comment( Reflejo hogar Izqda)
   			Type ( 0 )
   			Conditions (
    				Headlight ( 0 )
    				Unit ( 0 )
    				)
   			FadeIn ( 0.1 )
   			FadeOut ( 0.1 )
   			Cycle ( 0 )
   			States ( 4
    				State (
     					Duration ( 0.1 )
     					LightColour ( 40fff080 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  90.0 90.0 90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				State (
     					Duration ( 0.1 )
     					LightColour ( 00000000 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  90.0 90.0 90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				State (
     					Duration ( 0.1 )
     					LightColour ( 40ffc080 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  90.0 90.0 90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
     				State (
     					Duration ( 0.1 )
     					LightColour ( 20807040 )
     					Position ( 0.0 0.313 -2.506 )
     					Azimuth (  90.0 90.0 90.0 )
     					Transition ( 0 )
     					Radius ( 2 )
     					)
    				)
   			)
  		)
	
ORTSFreightAnims
		(
		MSTSFreightAnimEnabled( 0 )
			FreightAnimStatic
			(
			SubType( Default )
			Shape( "RN060-4008FAn1.s" )
			Offset( 0.0, 0.0, 0.0 )
		)
			FreightAnimStatic
			(
			SubType( Default )
			Shape( "RN060-4008FAn2.s" )
			Offset( 0.0, 0.0, 0.0 )
		)
	)

Sound ( "0604013_eng.sms" )
)

Engine ( RN060-4008  
	Effects (
  		SteamSpecialEffects
  		(


   			WhistleFX
   			(
    				0 3.984 -4.376
    				0 1 0
    				0.2
   				)

   			SafetyValvesFX
   			(
    				0 3.527 -0.821
    				0 1.2 0
    				0.3
   				)

   			StackFX
   			(
    				0 4.408 2.906
    				0 1 0
    				0.5
   				)

   			DrainpipeFX
   			(
    				-1.05 1.11 -3.886
    				-0.4 -1 -0.2
   				0.15
   				)

   			CylindersFX
   			(
    				-1.098 0.277 -0.746
    				-0.9 0.05 0.22
    				0.25
   				)

   			CylindersFX
   			(
    				1.098 0.277 -0.746
    				0.9 0.05 0.22 
    				0.25
   				)
			
			CylindersFX
   			(
    				-1.098 0.277 4.158
    				-0.9 0.05 0.22
    				0.25
   				)

   			CylindersFX
   			(
    				1.098 0.277 4.158
    				0.9 0.05 0.22 
    				0.25
   				)
  			)
 		)

	Comment(BOILER - POWER - FORCE)
	
	Wagon ( RN060-4008 )
	IsTenderRequired( 1 )	
	Type ( Steam )
	MaxPower ( 931.5kW )
	MaxForce ( 139.92kN )
	MaxVelocity ( 47mph )
	WheelRadius ( 0.600m )
	Sanding ( 1e9mph )
	NumWheels ( 6 )
	ORTSSteamLocomotiveType( Compound )

	Comment ("Congifuración de la caldera")

	BoilerLength ( 4.5m )
	BoilerVolume ( 300.2 )
	BoilerEffectivity ( 1.05 )
	DraftingEffect ( 1.01 )
	BoilerResponsiveness ( 1.0 )
	CoalBurnage ( 2.71lb/hp/h )
	MaxBoilerOutput ( 18600lb/h )
	ExhaustLimit ( 16640lb/h )
	ORTSSteamBoilerType( Superheated )
	ORTSEvaporationArea( 1306.83 )
	ORTSSuperheatArea ( 401.27 )
	ORTSGrateArea( 26.05 )
	ORTSBoilerEvaporationRate( 17.4 )
	ORTSBoilerEfficiency( 5.0 0.90  40.0 0.80  80 0.70  120 0.60  160.0  0.50 )

	Comment ("Cilindros")

	NumCylinders ( 2 )
	CylinderStroke ( 23.62in )
	CylinderDiameter ( 15.75in )
	CylinderVolume ( 11.72 )
	CylinderEffectivity ( 1.37 )
	LPNumCylinders( 2 )
	LPCylinderStroke( 23.62in )
	LPCylinderDiameter( 23.62in )
	InjectorSizes ( 12mm 12mm )
	PrimingFactor ( 1 )
	BlastExponent ( 0.5 )
	ORTSCylinderPortOpening( 0.08 )
	ORTSCylinderEfficiencyRate( 1.275 )
	ORTSBurnRate( 0.0 10.0  2660.0 260.5  5729.0 564.0  7568.0 847.0  9607.0 1129.0  11406.0 1411.0  12965.0 1693.0  14285.0 1975.0  15371.0 2258.0  16210.0 2540.0  16809.0 2822.0  17168.0 3104.0  17292.0 3387.0 )

	Comment ("Presion y trabajo de la caldera")

	MaxBoilerPressure ( 184.9psi )
	MaxFireMass ( 833.6lb )
	IdealFireMass ( 521.0lb )
	MaxWaterMass ( 3740.3lb )  	
	ShovelCoalMass ( 2lb )
	SmokeCombustion ( 1 )
	SuperHeater ( 1.32 )
	SteamSmokeUnitsPerPoundOfFuel( 1 )
	SteamMaxSmokeUnitsReleaseRate( 10 )
	SteamFiremanMaxPossibleFiringRate ( 3386.5 )
	ORTSSteamFiremanMaxPossibleFiringRate( 3386.5lb/h )

	Comment ("Capacidad del tender")

	MaxTenderCoalMass ( 9921lb )
	MaxTenderWaterMass ( 33069lb )

	Comment ("Valvulas de seguridad")

	SafetyValvesSteamUsage ( 9600lb/h )
	SafetyValvePressureDifference( 5 )
	SteamGaugeGlassHeight( 9 )	
	MaxSteamHeatingPressure( 80 )

	Comment ("Consumo")
	
	BasicSteamUsage ( 650lb/h )
	BasicCoalUsage ( 260.5lb/h )
	SteamSmallestCutoff( 10 )
	NumberOfDamperSteps( 4 )
	ORTSFuelCalorific( 13000btu/lb )

	Comment(0 for live steam, 1 for exhaust steam)

	InjectorTypes( 0 1 )

	comment( min steam pressure, min water proportion, max water proportion  )
 
	InjectorLimits1 ( 50psi 0.6 1 )
	InjectorLimits2 ( 60psi 0 1 )
	CylinderCocksPowerEfficiency ( 0.9 )
	SteamCylinderCocksOperation( Manual )

	Comment ("Configuración de los frenos")

      TrainBrakesControllerMaxReleaseRate( 12 )
	TrainBrakesControllerMaxApplicationRate( 10 )
	TrainBrakesControllerEmergencyApplicationRate( 35 )
	TrainBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMaxSystemPressure( 70 )
	TrainBrakesControllerMaxPressureDropInNormalApplication( 70 )

	EngineBrakesControllerHasProportionalBrake( 1 )
      EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 6 )
	EngineBrakesControllerMaxReleaseRate( 6 )
	EngineBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 70 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
      BrakesEngineControllers( "Hand, Train, Independent" )

	Comment ( "Tipo de regulador" )

	RegulatorValveType( Single_port )
	RegulatorMainValveExponent( 1 )
	
	SteamBlowerEffectExponent( 0.9 )
	SteamBlowerEfficiencyExponent( 1.1 )
	SteamBlowerMaxSteamUsageRate( 500 )	
	comment( lbs/h )
	SteamBlowerMaxProportionOfBlastEffect( 0.15 )

	AirBrakesAirCompressorPowerRating( 3.5 )
	AirBrakesMainMinResAirPressure( 0 )
	AirBrakesMainMaxResAirPressure( 110 )	
	AirBrakesMainResVolume( 8 )
	AirBrakesCompresorRestartPressure( 95 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.25 )

	CabView ( FS_GR740_2.cvf )

	HeadOut (  1.58 2.873 -5.322 )

        EngineControllers (
            comment( Engine controls )
        
            Regulator ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.75 0.75 0.015 0 
                NumNotches( 0 )
            )
            Brake_Train ( 0 1 0.015 0.65 
                NumNotches( 3
                    Notch(0     1 TrainBrakesControllerReleaseStart )
                    Notch(0.4   1 TrainBrakesControllerSelfLapStart )
                    Notch(0.5   1 TrainBrakesControllerApplyStart )
                )
            )
            
		Brake_Engine ( 0 1 0.0125 0
                NumNotches( 3
                    Notch(0    1 EngineBrakesControllerReleaseStart )
                    Notch(0.45 1 EngineBrakesControllerHoldStart )
                    Notch(0.5  1 EngineBrakesControllerApplyStart )
			)
		)
		Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.025 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1 
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            WaterScoop ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            Headlights( 0 1 0 )
        )
	comment(fire temp, fire mass, water mass, boiler pressure,
		water level, tender_water_mass, tender_coal_mass,
		smoke_quantity, fire_condition, coal quality )

	EngineVariables( 850 538.1 3003.9 184.9 0 0 0 200 1 1 )

	Sound ( "0604013_cab.sms" )

    	Name ( "Renfe 060-4008" )
 	Description (
 	"Autores:\n\n"+
	"Modelo 3d y Sonidos: Vicente Ramón Andreu Sanjuan\n\n"+
	"Texturas: Jesús Brau Martinez\n\n"+
	"Modificaciones fichero eng: José Maria Lozano Gallardo\n\n"+
	"Modificaciones luces: Arturo Ares Fernandez\n\n"+
	"Modificaciones Bounding box: Julio Gomez Diaz\n\n"+
	"Locomotoras y Tenders:\n\n"+
	"Central de Aragón 61-69\n\n"+
	"RENFE 060-4001/060-4009\n\n"+
	"Constructor: Henschel et Sonhn - Cassel 1912 - 1927/28 \n\n"+
	"En 1912 el Ferrocarril Central de Aragón adquirio tres locomotoras con el sistema Mallet para reforzar los servicios de mercancias entre Valencia y"+ 
	"Calatayud, apoyando en este cometido a las locomotoras ya existentes de las series 41-44 y 51-54."+
	"Eran practicamente iguales a la serie 51-54. RENFE 060/4011-4014, con la diferencia de que las nº 51-54 trabajaban con vapor"+
	"saturado mientras que las nº 61-69 iban provistas de recalentador de vapor, eran tambien ligeramente inferiores y llevaban"+ 
	"corredera plana en todos los cilindros.\n\n"
	"En 1927, ante el previsible aumento de tráfico derivado de la inauguración del trayecto Calatayud-Burgos del Santander-Mediterráneo,"+ 
	"el Ferrocarril Central de Aragón decidió adquirir seis locomotoras mas de este modelo,  con la unica diferencia que las nuevas ya"+
	"llevaban incorporado alumbrado electrico.\n\n" 
     	"Destinadas en el deposito de Valencia-Alameda, la serie completa llegó a RENFE, siendo trasladadas al deposito de Valencia-Termino,"+ 
	"donde prestaron servicio principalmente en la linea de Valencia - Utiel y ocasionalmente en la de Valencia - Jativa -La Encina, aunque"+
	"al final de su vida activa, tambien se las localizó efectuando trenes en la linea Alicante-Murcia.\n\n"+
	"Tras su baja, a finales de los 60, fueron apartadas en  Murcia - Zaraiche y desguazadas, no quedando preservada ninguna locomotora de esta serie.\n\n"
	) 
	EngineOperatingProcedures (
	"To move forward\n"+
	"1.	Press the W key several times to move the Reverser to full Forward.\n"+
	"2.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"3.	Press the D key to increase the Regulator setting.\n"+  
	"4.	As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+
	"To slow the train\n"+
	"1.	Press the A key to move the Regulator to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n"+
	"2. To hold the brakes at their current setting, lower the brake lever until it's in its middle (Neutral) position, by pressing the ; (SEMICOLON) key.\n\n"+
	"To release the train brakes\n"+
	"1. Press  the ; (SEMICOLON) key to release the train brakes.\n"+
	"2. When the brakes are released, raise the brake lever until it's in its middle (Neutral) position, by pressing the ' (APOSTROPHE) key.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+ 
	"2.	Press the S key several times to move the Reverser to the full Reverse position.\n"+
	"4.	Press the ; (SEMICOLON) key to release the brakes.\n"+
	"5.	Slowly advance the regulator (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the \"permission to depart\" whistle.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window.\n\n"+
	"Firing commands (Automatic Fireman OFF in Options screen)\n"+
	"To add coal to the firebox\n"+
	"1. Press the F key to open the Firebox door.\n"+
	"2. Press the R key to increase the shoveling rate.\n\n"+
	"To stop adding coal to the fire\n"+
	"1. Press SHIFT+R to decrease the shoveling rate.\n"+
	"2. Press SHIFT+F to close the firebox door.\n\n"+
	"To operate the blower\n"+
	"1.	Press the N key to increase the blower.\n"+
	"2. Press SHIFT+N to decrease the blower.\n\n"+
	"To operate the dampers\n"+
	"1.	Press the M key to open the dampers.\n"+
	"2. Press SHIFT+M to close the dampers.\n\n"+
	"To inject water into the boiler\n"+
	"1.	Press the I key to turn on the steam to Injector 1.\n"+
	"(You can also press the O key to turn on the steam to Injector 2.)\n"+
	"2.	Press the K key to increase the water flow to Injector 1.\n"+
	"(To increase the water flow to Injector 2, press the L key.)\n\n"+
	"To stop boiler water injection\n"+ 
	"1. Press the I key to turn off the steam to Injector 1.\n"+
	"2. Press the O key to turn off the steam to Injector 2."
	)
)
