SIMISA@@@@@@@@@@JINX0D0t______

Wagon ( NORTE1722
 Type ( Engine )
 WagonShape ( NORTE1722.s )
 
 Size  ( 2.92m 4.34m 8m )
 CentreOfGravity ( 0m 1.7m 0.25m )
 Centre ( 0m 0m 0m )
 Mass ( 38.4t )

 InertiaTensor ( Box(2.92m 4.34m 7.5m) )

	Coupling (
		Type ( Bar )
		Spring (
			Stiffness ( 5e6N/m 5e6N/m )
			Damping ( 4e6N/m/s 4e6N/m/s)
			Break ( 2e7N 2e7N )
			r0 ( 95cm 20cm )
			)
		Velocity ( 0.1m/s )
		CouplingHasRigidConnection ()
		)

	Coupling (
		Type ( Automatic )
		Spring (
			Stiffness ( 4e6N/m 5e6N/m )
			Damping ( 1e6N/m/s 4e6N/m/s )
			Break ( 2e7N 2e7N )
			r0 ( 0.1cm 20cm )
		)
		Velocity ( -0.1m/s )
	)

comment (friction steam engine- lightweight rods- friction roller- 70 kmh- axles 3- weight 38,4-38,4 front area 7,5)

 Friction (
	3644.4N/m/s    -0.10    1.9mph    4.869N/m/s    1.998
  	5.1N/rad/s  1  -1rad/s  0  1
 )


Adheasion ( 0.30 0.76  0.79  0 )
DerailRailHeight (4cm)
DerailRailForce ( 2.5*38.4kN )
DerailBufferForce ( 1.2*2.5*38.4kN )


 BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Handbrake" )
 BrakeSystemType ( "Air_single_pipe" )
 MaxBrakeForce ( 52.72kN )
 MaxHandbrakeForce( 52kN )
 NumberOfHandbrakeLeverSteps( 100 )
 TripleValveRatio( 2.5 )
 MaxReleaseRate( 15 )
 MaxApplicationRate( 15 )
 MaxAuxilaryChargingRate( 15 )
 BrakeCylinderPressureForMaxBrakeBrakeForce( 70 )

  Lights ( 5
  Light (
   comment( Head Sphere of light)
   Type ( 1 )
   Conditions(
    Headlight ( 3 )
    Unit ( 2 )
    )
   Cycle ( 0 )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( d0ffffd5 )
     Position ( 0.0 3.30 3.0 )
     Transition ( 0 )
     Radius ( 100.0 )
     Angle ( 25.0 )
     )
    )
   )
  Light ( 
   comment( Head light main )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( ffffffb5 )
     Position ( 0.14 3.10 3.50 )
     Azimuth ( 0.0 0.0 5.0 )
     Transition ( 0 )
     Radius ( 0.7 )
     )
    )
   )

  Light (
   comment( Head light rigth )
   Type ( 0 )
   Conditions (
    Headlight ( 3 )
    Unit ( 2 )
    )
   FadeIn ( 0.5 )
   FadeOut ( 0.5 )
   Cycle ( 0 )
   States ( 1
    State (
     Duration ( 0.0 )
     LightColour ( 80ff0000 )
     Position ( 0.98 1.653 3.700 )
     Azimuth ( 0.0 -5.0 5.0 )
     Transition ( 0 )
     Radius ( 0.5 )
     )
    )
   )
  
  Light (
   comment( Bottom firelight rigth )
   Type ( 0 )
   Conditions (
    Headlight ( 0 )
    Unit ( 0 )
    )
   FadeIn ( 0.1 )
   FadeOut ( 0.1 )
   Cycle ( 0 )
   States ( 4
    State (
     Duration ( 0.1 )
     LightColour ( 40fff080 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  -90.0 -90.0 -90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 00000000 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  -90.0 -90.0 -90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 40ffc080 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  -90.0 -90.0 -90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 20807040 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  -90.0 -90.0 -90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    )
   )
  Light (
   comment( Bottom firelight left)
   Type ( 0 )
   Conditions (
    Headlight ( 0 )
    Unit ( 0 )
    )
   FadeIn ( 0.1 )
   FadeOut ( 0.1 )
   Cycle ( 0 )
   States ( 4
    State (
     Duration ( 0.1 )
     LightColour ( 40fff080 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  90.0 90.0 90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 00000000 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  90.0 90.0 90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 40ffc080 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  90.0 90.0 90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    State (
     Duration ( 0.1 )
     LightColour ( 20807040 )
     Position ( 0.0 0.6 -2.1 )
     Azimuth (  90.0 90.0 90.0 )
     Transition ( 0 )
     Radius ( 2 )
     )
    )
   )
  )
 Sound ( "..\\..\\380\\SOUND\\380Eng.sms" )
)

Engine ( NORTE1722  

 Effects (
  SteamSpecialEffects
  (


   WhistleFX
   (
    0 4 -2.83
    0 1 0
    0.05
   )

   SafetyValvesFX
   (
    0 3.36 -0.55
    0 1.2 0
    0.15
   )

   StackFX
   (
    0 4.36 2.78
    0 1 0
    0.2
   )

   DrainpipeFX
   (
    -1.05 1.11 -3.886
    -0.4 -1 -0.2
    0.05
   )

   CylindersFX
   (
    -0.50 0.37 2.65
    -0.7 0.25 -0.2 
    0.15
   )

   CylindersFX
   (
    0.50 0.37 2.65
    0.7 0.25 -0.2 
    0.15
   )
  )
 )

Comment(BOILER - POWER - FORCE)

 Wagon ( NORTE1722 )
 Type ( Steam )
IsTenderRequired( 1 )

MaxPower ( 373kW )
MaxForce ( 70.62kN )
MaxVelocity ( 42mph )
WheelRadius ( 0.762m )
NumWheels ( 3 )
ORTSSteamLocomotiveType( Simple )

BoilerLength (4.32m) 
BoilerVolume ( 256.5 )
BoilerEffectivity ( 1.00 )
BoilerResponsiveness ( 1.00 )
DraftingEffect ( 1.04 )
BlastExponent ( 0.50 )
CoalBurnage ( 5.98lb/hp/h )
MaxBoilerOutput ( 16836lb/h )
ExhaustLimit ( 14688lb/h )
ORTSSteamBoilerType ( Saturated )
ORTSEvaporationArea( 1194.26 )
ORTSGrateArea( 22.17 )
ORTSBoilerEvaporationRate( 15.5 )

NumCylinders ( 2 )
CylinderStroke ( 25.98in )
CylinderDiameter ( 19.02in )
CylinderVolume ( 17.08 )
CylinderEffectivity ( 1.13 )
MaxBoilerPressure ( 113.79psi )
ORTSCylinderPortOpening( 0.07 )
ORTSCylinderEfficiencyRate( 1 )
ORTSBurnRate( 0lb/h, 10lbs/h
			2280.0lb/h, 221.7lbs/h
			4703.0lb/h, 499lbs/h
			6730.0lb/h, 748lbs/h
			8552.0lb/h, 998lbs/h
			10151.0lb/h, 1247lbs/h
			11537.0lb/h, 1496lbs/h
			12717.0lb/h, 1746lbs/h
			13676.0lb/h, 1995lbs/h
			14428.0lb/h, 2245lbs/h
			14960.0lb/h, 2494lbs/h
			15284.0lb/h, 2744lbs/h
			15388.0lb/h, 2993lbs/h )

IdealFireMass ( 443.4lb )
MaxFireMass ( 709.4lb )
MaxTenderCoalMass ( 13426lb )
MaxTenderWaterMass ( 24251lb )
SteamFiremanMaxPossibleFiringRate ( 2993 )
ORTSSteamFiremanMaxPossibleFiringRate ( 3520lb/h )

MaxWaterMass ( 3196.4lb )
SteamGaugeGlassHeight ( 9 )
BasicSteamUsage ( 700lb/h )
BasicCoalUsage ( 221.7lb/h )
SafetyValvesSteamUsage ( 8800lb/h )
SafetyValvePressureDifference( 7 )
ORTSFuelCalorific( 13000btu/lb )
	
RegulatorValveType( Single_port )
RegulatorMainValveExponent ( 1 )

InjectorSizes ( 9mm 9mm )
	InjectorTypes( 0 0 ) 
	Injector1WaterValveVariance( .7 )
	Injector2WaterValveVariance( .7 )
	InjectorLimits1 ( 35psi 0.2 1 )
	InjectorLimits2 ( 35psi 0.2 1 )

 PrimingFactor ( 1 )
 ShovelCoalMass( 1lb )
 SteamSmokeUnitsPerPoundOfFuel( 0.5 )
 MaxSteamHeatingPressure( 80 )
 SteamMaxSmokeUnitsReleaseRate ( 1 )
 
 CylinderCocksPowerEfficiency( 0.8 )
 SteamCylinderCocksOperation( Manual )
 SteamSmallestCutoff( 0.20 )
 NumberOfDamperSteps( 4 )
 SteamBlowerEffectExponent( 0.9 )
 SteamBlowerEfficiencyExponent( 1.1 )
 SteamBlowerMaxSteamUsageRate( 500 )
 SteamBlowerMaxProportionOfBlastEffect( 0.15 )

comment(BRAKES)

 BrakesEngineBrakeType ( "Air_single_pipe"  )
 BrakesTrainBrakeType ( "Air_single_pipe" )
 BrakesEngineControllers( "Hand, Train, Independent" )
 AirBrakesAirCompressorPowerRating( 3 )
 AirBrakesMainMinResAirPressure( 0 )
 AirBrakesMainMaxAirPressure( 100 )
 AirBrakesMainResVolume( 8 )
 AirBrakesCompressorRestartPressure( 95 )
 AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.25 )

 TrainBrakesControllerMaxApplicationRate( 5 )
 TrainBrakesControllerMaxReleaseRate( 10 )
 TrainBrakesControllerEmergencyApplicationRate( 10 )
 TrainBrakesControllerMinSystemPressure( 0 )
 TrainBrakesControllerMaxSystemPressure( 70 )
 TrainBrakesControllerMaxPressureDropInNormalApplication( 70 )

 EngineBrakesControllerMaxApplicationRate( 6 )
 EngineBrakesControllerMaxReleaseRate( 6 )
 EngineBrakesControllerMinSystemPressure( 0 )
 EngineBrakesControllerMaxSystemPressure( 70 )
 EngineBrakesControllerHasProportionalBrake( 1 )
 EngineBrakesProportionalBrakeLag( 0.9 )  

 CabView ( "RN030-2224.cvf" )
 
 HeadOut ( 1.5 3 -4 )

        EngineControllers (
            Regulator ( 0 1 0.01 0 
                NumNotches( 0 )
            )
            Cutoff    ( -0.75 0.75 0.01 0 
                NumNotches( 0 )
            )
            Brake_Engine ( 0 1 0.0125 0
                NumNotches( 3
                    Notch(0    1 EngineBrakesControllerReleaseStart )
                    Notch(0.45 1 EngineBrakesControllerHoldStart )
                    Notch(0.5  1 EngineBrakesControllerApplyStart )
                )
            )            
            Brake_Train ( 0 1 0.0125 0.6 
                NumNotches( 4
                    Notch(0    1 TrainBrakesControllerReleaseStart )
                    Notch(0.4  1 TrainBrakesControllerSelfLapStart )
                    Notch(0.5  1 TrainBrakesControllerApplyStart )
                    Notch(0.9  1 TrainBrakesControllerEmergencyStart )
                )
            )
            Brake_Hand ( 0 1 0.0125 0 
                NumNotches( 0 )
            )
            FireDoor ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Sanding( 0 1 0 )
            Blower ( 0 1 0.025 0.2 
                NumNotches( 0 )
            )
            HeatingTap ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Shovel ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            DampersFront ( 0 1 0.1 1
                NumNotches( 0 )
            )
            DampersBack ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector1Steam ( 0 1 0 )
            Injector2Steam ( 0 1 0 )
            Injector1Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            Injector2Water ( 0 1 0.1 0 
                NumNotches( 0 )
            )
            CylinderCocks ( 0 1 1 )
            Whistle ( 0 1 0 )
            SmallEjectorOrCompressor( 0 1 1 )
            BellToggle( 0 1 0 )
            Headlights( 0 1 0 )
        )
 comment(fire temp, fire mass, water mass, boiler pressure,tender_water_mass, tender_coal_mass, smoke_quantity, fire_condition, coal quality )
 EngineVariables( 750 400 1525 108 0 0 0 200 1 )
 Sound ( "..\\..\\380\\SOUND\\380Cab.sms" )
 Name ( "NORTE1722" )
 
Description (
 "Autor: Jesus Brau Martinez\n\n"+
 "Locomotoras y Tenderes núms\n\n"+
 "AVT  78_85\n\n"+
 "Norte  1719_1726\n\n"+
 "RENFE  030_2223/030_2230\n\n"+
 "Constructor Sharp Stewart Año 1891\n\n"+
 "Construidas para la AVT llegaron el mismo año de su fusion con Norte\n\n"+
 "En la Compañia del Norte prestaron servicio hasta su Nacionalizacion y creacion de Renfe\n\n"+
 "En su etapa de Renfe prestaron excelentes servicios hasta su retirada a mediadosde los años 60. Hasta esa fecha realizaron toda clase de servicios pues fue una locomotora mixta, de pasajeros y mercancias, aunque a final de su vida util se vio relegada a trabajos de Piloto. Siempre operó en la zona de Valencia, Sagunto y alrededores\n\n" 
 )
 EngineOperatingProcedures (
 "To move forward\n"+
 "1. Press the W key several times to move the Reverser to full Forward.\n"+
 "2. Press the ; (SEMICOLON) key to release the train brakes.\n"+
 "3. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
 "4. Press the D key to increase the Regulator setting.\n"+  
 "5. As you accelerate, press the S key to slowly reduce the Reverser setting, then adjust the Regulator to maintain the desired speed.\n\n"+ 
 "To slow the train\n"+
 "1. Press the A key to move the Regulator to a lower setting.\n"+
 "2. Use the brakes to further reduce speed if desired.\n\n"+   
 "To apply the train brakes\n"+
 "1. Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
 "To release the train brakes\n"+
 "1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
 "To apply the locomotive brake\n"+
 "1. Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
 "To release the locomotive brake\n"+
 "1. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n\n"+
 "To back up\n"+
 "1. Bring your train to a full stop.\n"+
 "2. Press the S key several times to move the Reverser to the full Reverse position.\n"+
 "3. Press the ; (SEMICOLON) key to release the brakes.\n"+
 "4. Slowly advance the Regulator (D key).\n\n"+
 "To load and unload passengers\n"+
 "1. Stop at a station.\n"+
 "2. Press the ENTER key.\n"+
 "3. Wait for the \"permission to depart\" whistle.\n"+
 "TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
 "To couple to a car or locomotive\n"+
 "1. Coast into the unit at a very slow speed, about 4 Km/h.\n"+
 "TIP: To use the Coupling view, press the 6 key.\n"+
 "2. Press F9 to open the Train Operations window.\n"+
 "3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
 "4. Close the Train Operations window.\n\n"+
 "To uncouple from a car or locomotive\n"+
 "1. Press F9 to open the Train Operations window.\n"+
 "2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
 "3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
 "4. Click the green 'coupler' between the units you want to uncouple.\n"+
 "5. Click the Uncouple button.\n"+
 "6. Close the Train Operations window.\n\n"+
 "Firing commands (Automatic Fireman OFF in Options screen)\n"+
 "To add coal to the firebox\n"+
 "1. Press the F key to open the Firebox door.\n"+
 "2. Press the R key to increase the shoveling rate.\n\n"+
 "To stop adding coal to the fire\n"+
 "1. Press SHIFT+R to decrease the shoveling rate.\n"+
 "2. Press SHIFT+F to close the firebox door.\n"+
 "To operate the blower\n\n"+
 "1. Press the N key to increase the blower.\n"+
 "2. Press SHIFT+N to decrease the blower.\n\n"+
 "To operate the dampers\n"+
 "1. Press the M key to open the dampers.\n"+
 "2. Press SHIFT+M to close the dampers.\n\n"+
 "To inject water into the boiler\n"+
 "1. Press the I key to turn on the steam to Injector 1.\n"+
 "(You can also press the O key to turn on the steam to Injector 2.)\n"+
 "2. Press the K key to increase the water flow to Injector 1.\n"+
 "(To increase the water flow to Injector 2, press the L key.)\n\n"+
 "To stop boiler water injection\n"+
 "1. Press the I key to turn off the steam to Injector 1.\n"+
 "2. Press the O key to turn off the steam to Injector 2."
 )
)
