SIMISA@@@@@@@@@@JINX0D0t______

Wagon (RN250-017T
	Type ( Engine )
	
	                      comment (--- Modelo y medidas --- )
						  
	WagonShape ( RN250017T.s )
	FreightAnim ( 250INT.s 1 1 )
	Size ( 3.18m 5.52m 20m )
	CentreOfGravity ( 0m 1.75m 0m )
	Mass ( 124t )
	InertiaTensor ( Box (3.18m 5.52m 19.5m) )
	
	
	                          comment ( --- Enganches ---)
							  
	Coupling (
    Type ( Automatic )
    Spring (
    Stiffness ( 1e6N/m 5e6N/m )
    Damping ( 1e6N/m/s 1e6N/m/s )
    Break ( 5.1e7N 5.1e7N )
    r0 ( 10cm 20cm )
    )
    comment( CouplingHasRigidConnection (1) )
    Velocity ( 0.1m/s )
    )
    Buffers (
    Spring (
    Stiffness ( 1e6N/m 5e6N/m )
    Damping ( 1e6N/m/s 1e6N/m/s )
    r0 ( 10cm 20cm )
    )
    Centre ( 0.5 )
    Radius ( 1 )
    Angle ( 0.5deg )
    )
 
                 comment ( --- Adherencia, Fricción, Rozamiento... --- )
 
    Adheasion ( 0.2 0.4 2 0 )
    DerailRailHeight ( 10cm )
    DerailRailForce ( 2.5*124t )
    DerailBufferForce ( 1215.2kN )
	ORTSRadius ( 0.65m )
	ORTSMaximumWheelFlangeAngle ( 70deg )
	ORTSWheelFlangeLength ( 1.0in )
	ORTSLengthBogieCentre ( 35ft )
	ORTSLengthCouplerFace ( 19.95m )
	ORTSLengthCarBody ( 19.45m )
	ORTSNumberBogies ( 2 )
    ORTSNumberAxles ( 6 )
    Friction (
    1564.3N/m/s    -0.10    1.2mph    12.670N/m/s    1.826
    5.1N/rad/s  1  -1rad/s  0  1
    )

                    comment ( --- Frenos sección Wagon --- )
   
	BrakeEquipmentType ( "Triple_valve, Auxilary_reservoir, Emergency_brake_reservoir" )
    BrakeSystemType ( "Air_single_pipe" )
    MaxBrakeForce ( 170.12kN )
   
    EmergencyBrakeResMaxPressure( 71 )
	TripleValveRatio( 2.03 )
	MaxReleaseRate( 20 )
	MaxApplicationRate( 20 )
	MaxAuxilaryChargingRate( 20 )
	EmergencyResCapacity( 4 )
	EmergencyResChargingRate( 20 )
	BrakeCylinderPressureForMaxBrakeBrakeForce( 71 )
	

	EmergencyResVolumeMultiplier( 1.15 )
	BrakeAirPressureGainInResForOnePoundFromPipe( 0.25 )

	BrakeDistributorFullServicePressure( 82 )
	BrakeDistributorMaxAuxilaryResPressure( 110 )
	BrakeDistributorEmergencyResPressure( 110 )
	BrakeDistributorReleaseRate( 10 )
	BrakeDistributorApplicationRate( 15 )
	BrakeDistributorTrainPipeControlRatio( 2.03 )
	BrakeDistributorNormalFullReleasePressure( 110 ) 
	
	

	                   comment ( === VITA INTERIOR === )
	Inside (
	   PassengerCabinHeadPos ( 1.2 3.2 -4 )
	   RotationLimit ( 0 0 0 )
	   StartDirection ( 0 0 0 )
	   Sound ( "DB_BR120_Cab.sms" )
	)                         
	
	                         comment ( === LUCES === )

    Lights	( 40

		Light	(
			comment( Campo de alumbrado reducido )
			Type		( 1 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( 0.0 3.5 10.5)
					Transition ( 0 )
					Radius ( 100.0 )
					Angle ( 10.0 )
					)
				)
		)
		Light	(
			comment( Campo de alumbrado pleno )
			Type		( 1 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			Cycle	( 0 )
			FadeIn	( 0.5 )
			FadeOut	( 0.5 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 0.0 3.5 10.5)
					Transition ( 0 )
					Radius ( 200.0 )
					Angle ( 15.0 )
					)
				)
		)
		Light	(
			comment( Foco principal derecho Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( -0.09 3.85 9.24 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
        Light	(
			comment( Foco principal derecho Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -0.09 3.85 9.24 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
		Light	(
			comment( Foco principal izquierdo Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( 0.09 3.85 9.24 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
        Light	(
			comment( Foco principal izquierdo Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 0.09 3.85 9.24 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
		Light	(
			comment( Posicion Izq Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( 1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Izq Bright)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Der Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( -1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Der Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Izq Dim)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Izq Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( -0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Der Dim)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Der Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 3 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( 0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		                      comment ( Chispazos pantógrafo )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 5.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 20.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 6.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 3.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 -5.3 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 2 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 5.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 20.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 6.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 3.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 -5.45 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
					)
				)
			)

comment( LUCES CABINA TRASERA )

        Light	(
			comment( Foco principal derecho Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( -0.09 3.85 -9.24 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
        Light	(
			comment( Foco principal derecho Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -0.09 3.85 -9.24 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
				Light	(
			comment( Foco principal izquierdo Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( 0.09 3.85 -9.24 )
                    Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
        Light	(
			comment( Foco principal izquierdo Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 0.09 3.85 -9.24 )
                    Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
		Light	(
			comment( Posicion Izq Dim)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( 1.06 1.64 -9.48 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Izq Bright)
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 1.06 1.64 -9.48 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Der Dim )
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80FFFFFF )
					Position ( -1.06 1.64 -9.48 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Posicion Der Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 5 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -1.06 1.64 -9.48 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Izq Dim)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( 0.52 1.64 9.57 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Izq Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( 0.52 1.64 9.57 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Der Dim)
			Type		( 0 )
			Conditions	(
				Headlight ( 2 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( 80ff0000 )
					Position ( -0.52 1.64 9.57 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Der Bright )
			Type		( 0 )
			Conditions	(
				Headlight ( 3 )
				Unit ( 4 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( -0.52 1.64 9.57 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		
		                      comment ( Chispazos pantógrafo )
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 5.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 20.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 6.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 3.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 -90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 4.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 15.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 7.0 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.0 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( 11000000 )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 0.05 )
					LightColour ( ffaaaaff )
					Position ( 0.0 5.4 5.35 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
					)
				)
			)
		Light	(
			Type		( 0 )
			Conditions	(
				Headlight ( 4 )
				Unit ( 5 )
				Service ( 2 )
			)
			FadeIn	( 0 )
			FadeOut	( 0 )
			Cycle	( 0 )
			States	(	8     
				State	(
					Duration ( 5.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.3 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 20.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 2.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 6.0 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 3.0 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 1.1 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( 11000000 )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
				)
				State	(
					Duration ( 1.05 )
					LightColour ( ffaaaaff )
					Position ( 0.05 5.4 5.55 )
					Azimuth ( 0.0 -180 180 )
					Transition ( 0 )
					Radius ( 0.90 )
					Elevation ( 0 90 90 )
					)
				)
			)

comment( LUCES IA )

        Light	(
			comment( Foco principal derecho Bright )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -0.09 3.85 9.24 )
					Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
        Light	(
			comment( Foco principal izquierdo Bright )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 2 )
				)
			FadeIn	( 0.2 )
			FadeOut	( 0.6 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 0.09 3.85 9.24 )
                    Azimuth ( 0 0 0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                    )
				)
		)
        Light	(
			comment( Posicion Izq )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( 1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
        Light	(
			comment( Posicion Der )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 2 )
				Service ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( FFFFFFFF )
					Position ( -1.06 1.64 9.48 )
					Azimuth ( 0.0 0.0 0.0 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Izq )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 3 )
				Service ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( 0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)
		Light	(
			comment( Cola Roja Der )
			Type		( 0 )
			Conditions	(
			    Control ( 1 )
				Headlight ( 3 )
				Unit ( 3 )
				Service ( 2 )
				)
			FadeIn	( 0.1 )
			FadeOut	( 0.2 )
			Cycle	( 0 )
			States	(	1
				State	(
					Duration ( 0.0 )
					LightColour ( eeff0000 )
					Position ( -0.52 1.64 -9.57 )
					Azimuth ( -180 -180 -180 )
					Transition ( 0 )
					Radius ( 0.8 )
					
                              )
				)
		)

    )	                              
	
	Sound ( "DB_BR120_Eng.sms" )
)

	
	
Engine ( RN250-017T
	Wagon ( RN250-017T )
	Type ( Electric )
	MaxPower ( 4600kW )
	MaxForce ( 410kN )
	MaxContinuousForce ( 316kN ) 
	MaxVelocity ( 140kmh ) comment (a partir de septiembre de 1988, 140 kmh en 
	de viajeros por problemas en la suspensión. En régimen de mercancías, 100 kmh)
	
	MaxCurrent ( 2000A )
	WheelRadius ( 0.65m )
	Sanding ( 1e9mph )
	ORTSNumberAxles ( 6 )
	MaxSteamHeatingPressure ( 80psi )

	CabView ( "250.cvf" )
	HeadOut ( 1.7 3.3 8.0 )

    Comment (---Frenos sección motriz---)
	
    AirBrakesAirCompressorPowerRating( 2 )
	AirBrakesMainMinResAirPressure( 100 )
	AirBrakesMainMaxAirPressure( 140 )
	AirBrakesMainResVolume( 8 )
	AirBrakesAirCompressorWattage( 10000 )
	AirBrakesCompressorRestartPressure( 110 )
	AirBrakesAirUsedPerPoundsOfBrakePipePressure( 0.2 )
	AirBrakesIsCompressorElectricOrMechanical( 1 )

	EngineBrakesControllerDirectControlExponent( 1 )

	TrainBrakesControllerMinPressureReduction( 6 )
	EngineBrakesControllerHasProportionalBrake( 1 )
	EngineBrakesProportionalBrakeLag( 0.9 )
	EngineBrakesControllerMaxApplicationRate( 20 )
	TrainBrakesControllerMaxApplicationRate( 20 )
	EngineBrakesControllerMaxReleaseRate( 10 )
	TrainBrakesControllerMaxReleaseRate( 2 )
	EngineBrakesControllerEmergencyApplicationRate( 50 )
	TrainBrakesControllerEmergencyApplicationRate( 50 )
	EngineBrakesControllerMinSystemPressure( 0 )
	TrainBrakesControllerMinSystemPressure( 0 )
	EngineBrakesControllerMaxSystemPressure( 110 )
	TrainBrakesControllerMaxSystemPressure( 110 )
	EngineBrakesControllerEmergencyBrakeTimePenalty( 0 )
	TrainBrakesControllerEmergencyBrakeTimePenalty( 0 )
	EngineBrakesControllerFullServicePressureDrop( 28 )
	TrainBrakesControllerFullServicePressureDrop( 28 )

	DynamicBrakesMinUsableSpeed( 5 )
	DynamicBrakesMaximumEffectiveSpeed( 25 )
	DynamicBrakesMaximumForce( 251kN )
	DynamicBrakesResistorCurrentLimit ( 1000 )
	DynamicBrakesCutInSpeed( 8 )
	DynamicBrakesMaxAirBrakePressure ( 15 )
	DynamicBrakesFadingSpeed( 25 )
	DynamicBrakesDelayTimeBeforeEngaging ( 0 )
	DynamicBrakesMaximumSpeedForFadeOut ( 65 )
	DynamicBrakesEffectAtMaximumFadeOut( 0 )
	DynamicBrakesHigherSpeedCurveExponent( 1 )
	DynamicBrakesLowerSpeedCurveExponent( 1 )
	DynamicBrakesNumberOfControllerNotches( 8 )
	DynamicBrakeHasAutoBailOff( 1 )

	BrakesEngineBrakeType( "Air_single_pipe"  )
	BrakesTrainBrakeType( "Air_single_pipe" )
    BrakesEngineControllers( "Independent, Train, Dynamic" )
	
	ORTSEngineBrakeReleaseRate( 5bar/s )
    ORTSEngineBrakeApplicationRate( 5bar/s )

	EngineBrakesControllerDirectControlExponent( 1 )
	TrainBrakesControllerDirectControlExponent( -1 )
	
	DoesHornTriggerBell( 0 )

   

    comment(---Monitores---)
    EmergencyStopMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 0 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 0 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 1 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
    )

    AWSMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 7 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 0 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 0 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
    )

    VigilanceMonitor(
        MonitoringDeviceMonitorTimeLimit ( 60 )
        MonitoringDeviceAlarmTimeLimit ( 55 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 0 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 1 )
        MonitoringDeviceAppliesEmergencyBrake ( 0 )
        MonitoringDeviceAppliesCutsPower ( 0 )
        MonitoringDeviceAppliesShutsDownEngine ( 1 )
        MonitoringDeviceResetOnZeroSpeed ( 1 )
    )

    OverspeedMonitor(
        MonitoringDeviceMonitorTimeLimit ( 0 )
        MonitoringDeviceAlarmTimeLimit ( 0 )
        MonitoringDevicePenaltyTimeLimit ( 0 )
        MonitoringDeviceCriticalLevel ( 150 )
        MonitoringDeviceResetLevel ( 0 )
        MonitoringDeviceAppliesFullBrake ( 1 )
        MonitoringDeviceAppliesEmergencyBrake ( 1 )
        MonitoringDeviceAppliesCutsPower ( 1 )
        MonitoringDeviceAppliesShutsDownEngine ( 0 )
        MonitoringDeviceTriggerOnTrackOverspeed ( 1 )
        MonitoringDeviceTriggerOnTrackOverspeedMargin ( 10 )
        MonitoringDeviceResetOnZeroSpeed ( 1 )
        MonitoringDeviceResetOnResetButton ( 0 )
    )

    comment(---Controles---)

   EngineControllers (
		Throttle ( 0 1 0.1 0 
			NumNotches ( 16
				Notch ( 0.0	0  Dummy )
				Notch ( 0.062 0 Dummy )
				Notch ( 0.124 0 Dummy )
				Notch ( 0.186 0	Dummy )
				Notch ( 0.248 0 Dummy )
				Notch (	0.310 0 Dummy )
				Notch ( 0.372 0 Dummy )
				Notch ( 0.434 0 Dummy )
				Notch ( 0.496 0 Dummy )
				Notch ( 0.558 0 Dummy )
				Notch ( 0.620 0 Dummy )
                Notch ( 0.682 0 Dummy )	
                Notch ( 0.744 0 Dummy )	
                Notch ( 0.816 0 Dummy )	
                Notch ( 0.910 0 Dummy )	
                Notch ( 1 0 Dummy )				
			)
		)
		Brake_Engine (
			0 1 0.0125 0 
			NumNotches ( 12
				Notch ( 0 0  )
				Notch ( 0.10 0  )
				Notch ( 0.25 0  )
				Notch ( 0.35 0  )
				Notch ( 0.45 0  )
				Notch ( 0.55 0  )			
				Notch ( 0.65 0  )			
				Notch ( 0.75 0  )
				Notch ( 0.85 0  )
				Notch ( 0.95 0  )				
				Notch ( 0.98 0  )				
				Notch ( 1 0  )
			)
		)
        Brake_Train ( 0 1 0.0125 0.5 
            NumNotches ( 7
                Notch ( 0       0 TrainBrakesControllerReleaseStart )
                Notch ( 0.15	0 TrainBrakesControllerHoldLappedStart )
                Notch ( 0.25    1 TrainBrakesControllerGraduatedSelfLapLimitedHoldingStart )
                Notch ( 0.55    0 TrainBrakesControllerSuppressionStart )
                Notch ( 0.85     0 TrainBrakesControllerContinuousServiceStart )
                Notch ( 0.95    0 TrainBrakesControllerEmergencyStart )
				Notch ( 1 0 ) 
            )
        )
        Brake_Dynamic ( 0 1 0.0125 0 
            NumNotches( 10 
			    Notch ( 0	0 )
				Notch ( 0.10	0 )
				Notch ( 0.20	0 )
				Notch ( 0.30	0 )
				Notch ( 0.45	0 )
				Notch (	0.65	0 )
				Notch ( 0.75	0 )
				Notch ( 0.85	0 )
				Notch ( 0.95	0 )
				Notch ( 1	0 )
			)
        )
		
        DirControl ( -1 0 1 1 )
        BellToggle( 0 1 0 )
        AWS ( 0 1 0 )
        Sanding ( 0 1 0 )
        Horn ( 0 1 0 )
        Wipers ( 0 1 0 )
        EmergencyStopToggle( 0 1 0 )
        Vigilance ( 0 1 0 )
        PantographToggle1 ( 0 1 1 )
        PantographToggle2 ( 0 1 1 )
        Headlights ( 0 0.25 1 0 )
        BailOffButton( 0 1 0 )
    )
    
	Name ( "RN250-017 TAXI PA UN de Cargas" )
	  Sound ( "DB_BR120_Cab.sms" )
	  
	  
      Description (
	"Años de recepción: 1982 / 1985 \n"+
	"Disposición de ejes: C' C' \n"+
	"Peso en servicio: 124 t \n"+
	"Vel. máxima: 140 / 100 km/h \n"+
    "Tensión: 3.000 V = \n"+
	"Potencia continua:  4.600 kW \n"+
	"Número de motores:  2 dobles \n"+
	"Servicio: línea, viajeros y mercancías \n"+
	"Constructores: MTM, CAF, BBC, Krauss-Maffei \n\n"+
	
	
	"Modelo realizado por: Jesús BRAU MARTÍNEZ (2024) \n\n"+
	
	
	
      "UN POCO DE HISTORIA: \n\n"+
      "A finales de los años 70 Renfe decidió adquirir nuevas locomotoras de gran potencia y elevada 
	  velocidad máxima que sirvieran tanto para trenes de viajeros como de mercancías. \n\n"+
      "Renfe realizó un pedido de 35 locomotoras de la nueva serie 250. Las cinco primeras unidades 
	  fueron fabricadas en Alemania y Suiza por Krauss-Maffey y Brown-Boveri, mientras que las restantes
 	  se fabricaron en España por MTM y CAF bajo licencia. \n\n"+
      "La serie 250 se compuso finalmente de 40 locomotoras, las cinco últimas dotadas de tecnología chopper
	  (subserie 250-601 a 605), que se suministraron entre 1982 y 1987. Las cinco primeras fueron construidas
	  en Alemania y las restantes en España. \n\n"+
	  "Si bien parece que, en una primera intención, la idea era asignarlas al depósito de Oviedo para 
	  servicio en Pajares, tras las pruebas efectuadas con esta serie y con las 251, fueron éstas últimas las
	  elegidas, quizás por la mejor inscripción en curva, como consecuencia del excelente diseño del
	  bogie central, y por estar dotadas todas ellas de equipo chopper. Lo cierto es que estuvieron asignadas
	  siempre a los depósitos de Barcelona y de Valencia al que, finalmente, fue a parar toda la serie. 
	  Su librea de origen fue la azul-amarilla, mientras que las cinco chopper lucieron la decoración
	  estrella \n\n"+   
      "Durante sus primeros años remolcaron muchos trenes de viajeros por su posibilidad de circular, 
	  a partir de 1986, a 160 Km/h. Sin embargo, dados sus complejos problemas mecánicos, se redujo su velocidad
	  máxima  a 140 km/h y, poco a poco, pasaron a remolcar sólo trenes de mercancías a 100 km/h y con una fiabilidad
	  del 50 por ciento. \n\n"
    )
	
	
	
        EngineOperatingProcedures (
        "To move forward\n"+
		
		
	"Al introducir los nuevos Script,s el arranque de la locomotora será más real, 
	   para ello tendremos que seguir los siguientes pasos:\n"+
    "1. Subir el Pantógrafo pulsando la tecla "P" o desde la cabina haciendo clic sobre la palanca
	situada a la parte inferior izquierda.\n"+
    "2. Accionar el Disyuntor extrarrápido para ello la combinación de las teclas es "Shift+O" 
	o accionar la palanca del mismo (parte inferior izquierda,
       a la palanca del pantógrafo)\n"+
    "3. Accionar el reenganche pulsando la tecla "O".\n"+
    "4. Continuar como de costumbre, aflojando frenos, colocando inversor en la posición deseada
	(adelante o atrás) y metiendo puntos de tracción en el regulador. \n"+ 
				
		
    "1. The pantograph has been raised for you. (If it is not up for some reason, press the P key to raise it.)\n"+
	"2.	Press the W key to move the Reverser to Forward.\n"+
	"3.	Press the ; (SEMICOLON) key to release the train brakes.\n"+
	"4. Press the [ (LEFT BRACKET) key to release the locomotive brake.\n"+
	"5.	Press the D key to move increase the Throttle setting.\n\n"+  
	"To slow the train\n"+
	"1.	Press the A key to move the throttle to a lower setting.\n"+
	"2.	Use the brakes to further reduce speed if desired.\n\n"+
	"To apply the train brakes\n"+
	"1.	Press the ' (APOSTROPHE) key to apply the train brakes.\n\n"+
	"To release the train brakes\n"+
	"1. Press the ; (SEMICOLON) key to release the train brakes.\n\n"+
	"To bail off the train brakes on the locomotive\n"+
	"1. Press the / (FORWARD SLASH) key.\n\n"+
	"To apply the locomotive brake\n"+
	"1.	Press the ] (RIGHT BRACKET) key to apply the locomotive brake.\n\n"+
		"To release the locomotive brake\n"+
	"1. Press the [ (LEFT BRACKET) to release the locomotive brake.\n\n"+
	"To activate emergency braking\n"+
	"1.	Press the A key to reduce the throttle to Idle.\n"+
	"2.	Press the BACKSPACE key to activate emergency braking.\n\n"+
	"To back up\n"+
	"1.	Bring your train to a full stop.\n"+
	"2.	Press the S key to move the Reverser to the Reverse position.\n"+
	"3.	Press the ; (SEMICOLON) key and the [ (LEFT BRACKET) key to release the brakes.\n"+
	"4.	Slowly advance the throttle lever (D key).\n\n"+
	"To load and unload passengers\n"+
	"1. Stop at a station.\n"+
	"2. Press the ENTER key.\n"+
	"3. Wait for the 'permission to depart' signal.\n"+
	"TIP: Use the Next Station driving aid (F10) to monitor loading and unloading.\n\n"+
	"To couple to a car or locomotive\n"+
	"1. Coast into the unit at a very slow speed, about 2 mph.\n"+
	"TIP: To use the Coupling view, press the 6 key.\n"+
	"2. Press F9 to open the Train Operations window.\n"+
	"3. If the icon for the unit you coupled to is red, the handbrake is on. Double-click the car to release the handbrake.\n"+
	"4. Close the Train Operations window.\n\n"+
	"To uncouple from a car or locomotive\n"+
	"1. Press F9 to open the Train Operations window.\n"+
	"2. Double-click a unit in the part of the train you want to uncouple from the locomotive, to set the handbrake.\n"+
	"3. Double-click the coupler between the units you want to uncouple and the rest of the train.\n"+
	"4. Close the Train Operations window."
        ) 
)
